{"text_format":"1","workbook":"xlsx","n_sheets":40,"sheets":["仕様書","対象製品ﾘｽﾄ","AF","AFM","AFD","AFG","AR","AR□M","AL","AW","AWM","AWD","ARG","AWG","ARP","AV-A","AFF","AM","AMD","IDG","AMK","PF3A7","PF3A8","VP☐E","VP□R","JSXM","VPX","Y□(T)","VHS","E□00","E□00L","E□00T","Y□10","Y□4","IS10M","IS10T","IS10L","IS10E","E□00E","AKM"],"not_rendered":{"charts":0,"images":109,"macros":1,"external_links":1,"defined_names":74,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"仕様書","index":0,"n_rows":54,"n_cols":50,"rows_kept":54,"cut":false,"hidden":false,"merged":[[52,32,52,33],[52,34,52,37],[52,38,52,39],[52,40,52,43],[52,44,52,46],[52,47,52,49],[51,44,51,46],[51,47,51,49],[52,2,52,5],[52,6,52,7],[52,8,52,11],[52,12,52,13],[52,14,52,17],[52,18,52,20],[52,21,52,23],[52,28,52,31],[51,32,51,33],[51,34,51,35],[51,36,51,37],[51,38,51,39],[51,40,51,41],[51,42,51,43],[51,14,51,15],[51,16,51,17],[51,18,51,20],[51,21,51,23],[51,28,51,29],[51,30,51,31],[51,2,51,3],[51,4,51,5],[51,6,51,7],[51,8,51,9],[51,10,51,11],[51,12,51,13],[46,10,47,14],[46,36,47,40],[49,2,49,5],[49,6,49,23],[49,28,49,31],[49,32,49,49],[43,3,43,10],[43,14,43,22],[43,31,43,38],[43,41,43,47],[44,3,44,10],[44,14,44,22],[44,31,44,38],[44,41,44,47],[41,3,41,10],[41,14,41,22],[41,31,41,38],[41,41,41,47],[42,3,42,10],[42,14,42,22],[42,31,42,38],[42,41,42,47],[39,3,39,10],[39,14,39,22],[39,31,39,38],[39,41,39,47],[40,3,40,10],[40,14,40,22],[40,31,40,38],[40,41,40,47],[36,41,36,47],[37,3,37,10],[37,14,37,22],[37,31,37,38],[37,41,37,47],[38,3,38,10],[38,14,38,22],[38,31,38,38],[38,41,38,47],[34,3,34,10],[34,15,34,22],[34,31,34,38],[35,3,35,10],[35,31,35,38],[36,3,36,10],[36,14,36,22],[36,31,36,38],[32,3,32,10],[32,15,32,22],[32,31,32,38],[33,3,33,10],[33,15,33,22],[33,31,33,38],[30,3,30,10],[30,15,30,22],[30,31,30,38],[31,3,31,10],[31,15,31,22],[31,31,31,38],[28,3,28,10],[28,15,28,22],[28,31,28,38],[29,3,29,10],[29,15,29,22],[29,31,29,38],[26,3,26,10],[26,15,26,22],[26,31,26,38],[27,3,27,10],[27,15,27,22],[27,31,27,38],[23,2,23,4],[23,30,23,32],[24,3,24,10],[24,15,24,22],[24,31,24,38],[25,3,25,10],[25,15,25,22],[25,31,25,38],[4,22,4,23],[5,2,5,4],[5,5,5,9],[5,10,5,12],[5,13,5,16],[5,17,5,19],[5,20,5,23],[4,2,4,4],[4,5,4,9],[4,10,4,12],[4,13,4,16],[4,17,4,19],[4,20,4,21],[0,2,0,4],[0,5,0,23],[2,15,2,16],[2,17,2,18],[3,2,3,4],[3,5,3,9],[3,10,3,12],[3,13,3,16],[3,17,3,19],[3,20,3,23]]}
[null,null,"SMC株式会社",null,null,"F.R.L. エアコンビネーション 組合せ簡易特注品仕様書"]
[null,null,"お客様ご記入欄",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"記入例"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"作成日",null,null,null,"年",null,"月",null,"日"]
[null,null,"貴社名",null,null,null,null,null,null,null,"貴部署名",null,null,null,null,null,null,"ご担当者名"]
[null,null,"ＴＥＬ",null,null,null,null,null,null,null,"ＦＡＸ",null,null,null,null,null,null,"リピート"]
[null,null,"装置名(NO.)",null,null,null,null,null,null,null,"図　番",null,null,null,null,null,null,"工番・作番"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"組合せ表",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"組合せ表"]
[null,null,"組付\n位置","品番記載欄",null,null,null,null,null,null,null,"向き\n指定",null,null,"組付\n位置","品番記載欄",null,null,null,null,null,null,null,"向き\n指定",null,null,null,null,null,null,"組付\n位置","品番記載欄",null,null,null,null,null,null,null,"向き\n指定"]
[null,null,{"$f":"IF(D26=\"\",\"\",1)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P26=\"\",\"\",21)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"E300-04-D"]
[null,null,{"$f":"IF(D27=\"\",\"\",2)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P27=\"\",\"\",22)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"Y300T-D"]
[null,null,{"$f":"IF(D28=\"\",\"\",3)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P28=\"\",\"\",23)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"AF30-03-D"]
[null,null,{"$f":"IF(D29=\"\",\"\",4)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P29=\"\",\"\",24)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"Y300T-D"]
[null,null,{"$f":"IF(D30=\"\",\"\",5)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P30=\"\",\"\",25)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"Y310-02-D",null,null,null,null,null,null,null,"B"]
[null,null,{"$f":"IF(D31=\"\",\"\",6)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P31=\"\",\"\",26)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"Y300T-D"]
[null,null,{"$f":"IF(D32=\"\",\"\",7)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P32=\"\",\"\",27)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"AR30-03-D"]
[null,null,{"$f":"IF(D33=\"\",\"\",8)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P33=\"\",\"\",28)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"Y300T-D"]
[null,null,{"$f":"IF(D34=\"\",\"\",9)","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P34=\"\",\"\",29)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"IS10M-30-D"]
[null,null,{"$f":"IF(D35=\"\",\"\",10)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"Y300T-D"]
[null,null,{"$f":"IF(D36=\"\",\"\",11)","v":""},null,null,null,null,null,null,null,null,null,null,null,"同梱製品",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,"AL30-03-D",null,null,null,null,null,null,null,null,null,"同梱製品"]
[null,null,{"$f":"IF(D37=\"\",\"\",12)","v":""},null,null,null,null,null,null,null,null,null,null,null,"品番記載欄",null,null,null,null,null,null,null,null,"数量",null,null,null,null,null,null,12,"Y300T-D",null,null,null,null,null,null,null,null,null,"品番記載欄",null,null,null,null,null,null,"数量"]
[null,null,{"$f":"IF(D38=\"\",\"\",13)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,"VHS30-03-D",null,null,null,null,null,null,null,null,null,"KQ2L08-03AS",null,null,null,null,null,null,2]
[null,null,{"$f":"IF(D39=\"\",\"\",14)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,"Y300T-D",null,null,null,null,null,null,null,null,null,"KQ2H06-02AS",null,null,null,null,null,null,1]
[null,null,{"$f":"IF(D40=\"\",\"\",15)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"E300-04-D"]
[null,null,{"$f":"IF(D41=\"\",\"\",16)","v":""}]
[null,null,{"$f":"IF(D42=\"\",\"\",17)","v":""}]
[null,null,{"$f":"IF(D43=\"\",\"\",18)","v":""}]
[null,null,{"$f":"IF(D44=\"\",\"\",19)","v":""}]
[null,null,{"$f":"IF(D45=\"\",\"\",20)","v":""}]
[]
[null,null,null,null,null,null,null,null,null,null,"以下SMC担当記入欄",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"以下SMC担当記入欄"]
[]
[null,null,"ご発注品番　(この品番で手配下さるよう、お願い申し上げます。)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ご発注品番　(この品番で手配下さるよう、お願い申し上げます。)"]
[null,null,"簡易特注品番",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"簡易特注品番",null,null,null,"AC＊＊X-＊＊＊＊＊-D"]
[]
[null,null,"客先コード",null,null,null,"U/C",null,null,null,"部署ｺｰﾄﾞ",null,null,null,"担当ｺｰﾄﾞ",null,null,null,"イメージ登録No.",null,null,null,null,null,null,null,null,null,"客先コード",null,null,null,"U/C",null,null,null,"部署ｺｰﾄﾞ",null,null,null,"担当ｺｰﾄﾞ",null,null,null,"イメージ登録No."]
[null,null,"ＦＡＸ手配時記入欄",null,null,null,"客先注番",null,null,null,null,null,"客先納期",null,null,null,null,null,"ＳＭＣ手配Ｎｏ",null,null,null,null,null,null,null,null,null,"ＦＡＸ手配時記入欄",null,null,null,"客先注番",null,null,null,null,null,"客先納期",null,null,null,null,null,"ＳＭＣ手配Ｎｏ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"シリアルNo.AC※※X-D_27",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"X54","v":"シリアルNo.AC※※X-D_27"}]

{"sheet":"対象製品ﾘｽﾄ","index":1,"n_rows":186,"n_cols":7,"rows_kept":186,"cut":false,"hidden":false,"merged":[[18,1,21,1],[18,4,21,4],[18,5,21,5],[18,6,21,6],[173,6,175,6],[173,1,175,1],[84,1,88,1],[84,4,88,4],[84,5,88,5],[84,6,88,6],[76,1,78,1],[76,4,78,4],[76,5,78,5],[125,1,129,1],[125,4,129,4],[125,5,129,5],[160,6,164,6],[125,6,129,6],[120,5,124,5],[120,6,124,6],[170,1,172,1],[170,5,172,5],[170,4,172,4],[170,6,172,6],[89,6,93,6],[173,4,175,4],[173,5,175,5],[115,4,119,4],[115,5,119,5],[110,1,114,1],[110,4,114,4],[89,1,93,1],[89,4,93,4],[89,5,93,5],[98,1,99,1],[98,4,99,4],[115,1,119,1],[100,1,102,1],[100,4,102,4],[100,5,102,5],[98,5,99,5],[145,1,149,1],[145,4,149,4],[145,5,149,5],[140,1,144,1],[135,1,139,1],[135,4,139,4],[135,5,139,5],[48,1,50,1],[48,4,50,4],[51,1,53,1],[51,4,53,4],[48,5,50,5],[51,5,53,5],[57,1,60,1],[57,4,60,4],[57,5,60,5],[54,1,56,1],[54,4,56,4],[54,5,56,5],[103,4,105,4],[103,5,105,5],[103,1,105,1],[94,1,97,1],[42,4,44,4],[45,4,47,4],[42,5,44,5],[45,5,47,5],[57,6,60,6],[79,1,83,1],[79,4,83,4],[79,5,83,5],[61,1,65,1],[66,1,70,1],[61,4,65,4],[61,5,65,5],[66,4,70,4],[66,5,70,5],[71,4,75,4],[71,1,75,1],[66,6,68,6],[71,6,73,6],[61,6,63,6],[71,5,75,5],[165,1,169,1],[155,1,159,1],[150,1,154,1],[150,4,154,4],[150,5,154,5],[165,4,169,4],[165,5,169,5],[165,6,169,6],[155,4,159,4],[155,5,159,5],[155,6,159,6],[160,1,164,1],[150,6,154,6],[160,5,164,5],[160,4,164,4],[28,1,30,1],[145,6,149,6],[130,4,134,4],[130,5,134,5],[130,6,134,6],[130,1,134,1],[94,4,97,4],[94,5,97,5],[94,6,97,6],[140,4,144,4],[140,5,144,5],[140,6,144,6],[28,4,30,4],[28,5,30,5],[37,6,41,6],[42,1,44,1],[45,1,47,1],[31,6,36,6],[31,4,36,4],[31,5,36,5],[31,1,36,1],[37,1,41,1],[37,4,41,4],[37,5,41,5],[103,6,105,6],[135,6,139,6],[4,5,9,5],[4,4,9,4],[4,6,9,6],[4,1,9,1],[10,4,13,4],[10,5,13,5],[10,1,13,1],[10,6,13,6],[14,1,17,1],[14,4,17,4],[14,5,17,5],[14,6,17,6],[115,6,119,6],[120,1,124,1],[120,4,124,4],[22,4,27,4],[22,5,27,5],[22,6,27,6],[22,1,27,1],[110,5,114,5],[110,6,114,6],[98,6,99,6]]}
[null,"対象製品ﾘｽﾄ"]
[]
[null,"FRL-D　対象製品"]
[null,"品　名","型式","適用AC","種　類","選択範囲","注記"]
[null,"ｴｱﾌｨﾙﾀ","AF20-D","AC20-D","製品","カタログに準拠\n（但し、AF用ブラケットは選択できません。）"]
[null,null,"AF30-D","AC30-D"]
[null,null,"AF40-D","AC40-D"]
[null,null,"AF40-06-D","AC40-06-D"]
[null,null,"AF50-D","AC50-D\nAC60-D"]
[null,null,"AF60-D","AC50-D\nAC60-D"]
[null,"ﾐｽﾄｾﾊﾟﾚｰﾀ","AFM20-D","AC20-D","製品","カタログに準拠\n（但し、AFM用ブラケットは選択できません。）"]
[null,null,"AFM30-D","AC30-D"]
[null,null,"AFM40-D","AC40-D"]
[null,null,"AFM40-06-D","AC40-06-D"]
[null,"ﾏｲｸﾛﾐｽﾄｾﾊﾟﾚｰﾀ","AFD20-D","AC20-D","製品","カタログに準拠\n（但し、AFD用ブラケットは選択できません。）"]
[null,null,"AFD30-D","AC30-D"]
[null,null,"AFD40-D","AC40-D"]
[null,null,"AFD40-06-D","AC40-06-D"]
[null,"ｳｫｰﾀｾﾊﾟﾚｰﾀ","AFG20-D","AC20-D","製品","カタログに準拠\n（但し、AFG用ブラケットは選択できません。）"]
[null,null,"AFG30-D","AC30-D"]
[null,null,"AFG40-D","AC40-D"]
[null,null,"AFG40-06-D","AC40-06-D"]
[null,"ﾚｷﾞｭﾚｰﾀ","AR20(K)-D","AC20-D","製品","カタログに準拠\n（但し、AR用ブラケット、パネルマウント用セットナットは選択できません。）"]
[null,null,"AR30(K)-D","AC30-D"]
[null,null,"AR40(K)-D","AC40-D"]
[null,null,"AR40(K)-06-D","AC40-06-D"]
[null,null,"AR50(K)-D","AC50-D\nAC60-D"]
[null,null,"AR60(K)-D","AC50-D\nAC60-D"]
[null,"ﾓｼﾞｭﾗﾀｲﾌﾟ共通給気形ﾚｷﾞｭﾚｰﾀ","AR20M(K)-D","AC20-D","製品","カタログに準拠\n（但し、AR□M用ブラケット、パネルマウント用セットナットは選択できません。）"]
[null,null,"AR30M(K)-D","AC30-D"]
[null,null,"AR40M(K)-D","AC40-D"]
[null,"ﾙﾌﾞﾘｹｰﾀ","AL20-D","AC20-D","製品","カタログに準拠\n（但し、AL用ブラケットは選択できません。）"]
[null,null,"AL30-D","AC30-D"]
[null,null,"AL40-D","AC40-D"]
[null,null,"AL40-06-D","AC40-06-D"]
[null,null,"AL50-D","AC50-D\nAC60-D"]
[null,null,"AL60-D","AC50-D\nAC60-D"]
[null,"ﾌｨﾙﾀﾚｷﾞｭﾚｰﾀ","AW20(K)-D","AC20-D","製品","カタログに準拠\n（但し、AW用ブラケット、パネルマウント用セットナットは選択できません。）"]
[null,null,"AW30(K)-D","AC30-D"]
[null,null,"AW40(K)-D","AC40-D"]
[null,null,"AW40(K)-06-D","AC40-06-D"]
[null,null,"AW60(K)-D","AC50-D\nAC60-D"]
[null,"ﾐｽﾄｾﾊﾟﾚｰﾀﾚｷﾞｭﾚｰﾀ","AWM20-D","AC20-D","製品","カタログに準拠\n（但し、AW用ブラケット、パネルマウント用セットナットは選択できません。）"]
[null,null,"AWM30-D","AC30-D"]
[null,null,"AWM40-D","AC40-D"]
[null,"ﾏｲｸﾛﾐｽﾄｾﾊﾟﾚｰﾀﾚｷﾞｭﾚｰﾀ","AWD20-D","AC20-D","製品","カタログに準拠\n（但し、AW用ブラケット、パネルマウント用セットナットは選択できません。）"]
[null,null,"AWD30-D","AC30-D"]
[null,null,"AWD40-D","AC40-D"]
[null,"圧力計内蔵ﾚｷﾞｭﾚｰﾀ","ARG20(K)-B","AC20-D","製品","カタログに準拠\n（但し、ARG用ブラケット、パネルマウント用セットナットは選択できません。）"]
[null,null,"ARG30(K)-B","AC30-D"]
[null,null,"ARG40(K)-B","AC40-D"]
[null,"圧力計内蔵ﾌｨﾙﾀﾚｷﾞｭﾚｰﾀ","AWG20(K)-B","AC20-D","製品","カタログに準拠\n（但し、AWG用ブラケット、パネルマウント用セットナットは選択できません。）"]
[null,null,"AWG30(K)-B","AC30-D"]
[null,null,"AWG40(K)-B","AC40-D"]
[null,"直動精密ﾚｷﾞｭﾚｰﾀ","ARP20(K)","AC20-D","製品","カタログに準拠\n（但し、ARP用ブラケット、パネルマウント用セットナットは選択できません。）"]
[null,null,"ARP30(K)","AC30-D"]
[null,null,"ARP40(K)","AC40-D"]
[null,"ｿﾌﾄｽﾀｰﾄｱｯﾌﾟﾊﾞﾙﾌﾞ","AV2000-A","AC20-D","製品","カタログに準拠\n（但し、AV用ブラケットは選択できません。）"]
[null,null,"AV3000-A","AC30-D"]
[null,null,"AV4000-A","AC40-D"]
[null,null,"AV5000-A","AC50-D\nAC60-D"]
[null,"ﾗｲﾝﾌｨﾙﾀ","AFF20-D","AC20-D","製品","カタログに準拠\n（但し、AFF用ブラケットは選択できません。）"]
[null,null,"AFF30-D","AC30-D"]
[null,null,"AFF40-D","AC40-D"]
[null,null,"AFF50-D","AC50-D\nAC60-D"]
[null,null,"AFF60-D","AC50-D\nAC60-D"]
[null,"ﾐｽﾄｾﾊﾟﾚｰﾀ","AM20-D","AC20-D","製品","カタログに準拠\n（但し、AM用ブラケットは選択できません。）"]
[null,null,"AM30-D","AC30-D"]
[null,null,"AM40-D","AC40-D"]
[null,null,"AM50-D","AC50-D\nAC60-D"]
[null,null,"AM60-D","AC50-D\nAC60-D"]
[null,"ﾏｲｸﾛﾐｽﾄｾﾊﾟﾚｰﾀ","AMD20-D","AC20-D","製品","カタログに準拠\n（但し、AMD用ブラケットは選択できません。）"]
[null,null,"AMD30-D","AC30-D"]
[null,null,"AMD40-D","AC40-D"]
[null,null,"AMD50-D","AC50-D\nAC60-D"]
[null,null,"AMD60-D","AC50-D\nAC60-D"]
[null,"ﾒﾝﾌﾞﾚﾝｴｱﾄﾞﾗｲﾔ","IDG20-D","AC20-D","製品","カタログに準拠\n（但し、IDG用ブラケットは選択できません。）"]
[null,null,"IDG30-D","AC30-D"]
[null,null,"IDG40-D","AC40-D"]
[null,"活性炭ﾌｨﾙﾀ","AMK20-D","AC20-D","製品","カタログに準拠\n（但し、AMK用ブラケットは選択できません。）"]
[null,null,"AMK30-D","AC30-D"]
[null,null,"AMK40-D","AC40-D"]
[null,null,"AMK50-D","AC50-D\nAC60-D"]
[null,null,"AMK60-D","AC50-D\nAC60-D"]
[null,"ﾃﾞｼﾞﾀﾙﾌﾛｰｽｲｯﾁ","PF3A7R5","AC20-D","製品","カタログに準拠"]
[null,null,"PF3A701","AC30-D"]
[null,null,"PF3A702","AC40-D"]
[null,null,"PF3A704","AC50-D\nAC60-D"]
[null,null,"PF3A708","AC50-D\nAC60-D"]
[null,"ﾃﾞｼﾞﾀﾙﾌﾛｰｽｲｯﾁ\n(圧力/温度ｾﾝｻ付)","PF3A8R5","AC20-D","製品","カタログに準拠"]
[null,null,"PF3A801","AC30-D"]
[null,null,"PF3A802","AC40-D"]
[null,null,"PF3A804","AC50-D\nAC60-D"]
[null,null,"PF3A808","AC50-D\nAC60-D"]
[null,"3ﾎﾟｰﾄ残圧排気弁ﾓｼﾞｭﾗ接続ﾀｲﾌﾟ\n（主弁位置検出機能なし）","VP346E","AC20-D","製品","カタログに準拠"]
[null,null,"VP546E","AC30-D"]
[null,null,"VP746E","AC40-D"]
[null,null,"VP946E","AC50-D\nAC60-D"]
[null,"3ﾎﾟｰﾄ残圧排気弁ﾓｼﾞｭﾗ接続ﾀｲﾌﾟ\n（主弁位置検出機能付き）","VP546R","AC30-D","製品","カタログに準拠"]
[null,null,"VP746R","AC40-D"]
[null,"ﾓｼﾞｭﾗ取付形\n2ﾎﾟｰﾄｿﾚﾉｲﾄﾞﾊﾞﾙﾌﾞ","JSXM2","AC20-D","製品","カタログに準拠"]
[null,null,"JSXM3","AC30-D"]
[null,null,"JSXM4","AC40-D"]
[null,"安全排気ﾊﾞﾙﾌﾞﾓｼﾞｭﾗ接続ﾀｲﾌﾟ","VPX406KT-A3","AC30-D","製品","カタログに準拠","サイレンサが必要な場合は、INA-25-100を選定ください。"]
[null,null,"VPX406KT-A4","AC40-D"]
[null,null,"VPX406KT-A6","AC50-D\nAC60-D"]
[]
[]
[null,"FRL-D スペーサ、アタッチメント"]
[null,"品　名","型式","適用AC","種類","選択範囲","注記"]
[null,"ｽﾍﾟｰｻ","Y200-D","AC20-D","ｽﾍﾟｰｻ","カタログに準拠"]
[null,null,"Y300-D","AC30-D"]
[null,null,"Y400-D","AC40-D"]
[null,null,"Y500-D","AC40-06-D"]
[null,null,"Y600-D","AC50-D\nAC60-D"]
[null,"ﾌﾞﾗｹｯﾄ付ｽﾍﾟｰｻ","Y200T-D","AC20-D","ｽﾍﾟｰｻ","カタログに準拠"]
[null,null,"Y300T-D","AC30-D"]
[null,null,"Y400T-D","AC40-D"]
[null,null,"Y500T-D","AC40-06-D"]
[null,null,"Y600T-D","AC50-D\nAC60-D"]
[null,"残圧抜き3ﾎﾟｰﾄ弁","VHS20-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","カタログに準拠"]
[null,null,"VHS30-D","AC30-D"]
[null,null,"VHS40-D","AC40-D"]
[null,null,"VHS40-06-D","AC40-06-D"]
[null,null,"VHS50-D","AC50-D\nAC60-D"]
[null,"配管ｱﾀﾞﾌﾟﾀ","E200-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","カタログに準拠"]
[null,null,"E300-D","AC30-D"]
[null,null,"E400-D","AC40-D"]
[null,null,"E500-D","AC40-06-D"]
[null,null,"E600-D","AC50-D\nAC60-D"]
[null,"L形配管ｱﾀﾞﾌﾟﾀ","E200L-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","カタログに準拠","下向きは、向き指定欄に「B」を入力してください。"]
[null,null,"E300L-D","AC30-D"]
[null,null,"E400L-D","AC40-D"]
[null,null,"E500L-D","AC40-06-D"]
[null,null,"E600L-D","AC50-D\nAC60-D"]
[null,"T形配管ｱﾀﾞﾌﾟﾀ","E200T-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","カタログに準拠"]
[null,null,"E300T-D","AC30-D"]
[null,null,"E400T-D","AC40-D"]
[null,null,"E500T-D","AC40-06-D"]
[null,null,"E600T-D","AC50-D\nAC60-D"]
[null,"T形ｽﾍﾟｰｻ","Y210-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","カタログに準拠","・下向きは、向き指定欄に「B」を入力してください。\n・従来品と面間互換タイプは準標準仕様「1」を選択してください。\n　その場合、組合せに制限がありますので、組合せ注意事項を\n　参照してください。"]
[null,null,"Y310-D","AC30-D"]
[null,null,"Y410-D","AC40-D"]
[null,null,"Y510-D","AC40-06-D"]
[null,null,"Y610-D","AC50-D\nAC60-D"]
[null,"ｸﾛｽｽﾍﾟｰｻ","Y24-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","カタログに準拠","従来品と面間互換タイプは準標準仕様「1」を選択してください。"]
[null,null,"Y34-D","AC30-D"]
[null,null,"Y44-D","AC40-D"]
[null,null,"Y54-D","AC40-06-D"]
[null,null,"Y64-D","AC50-D\nAC60-D"]
[null,"圧力ｽｲｯﾁ","IS10M-20-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","カタログに準拠","・下向きの取付けはできません。\n・従来品と面間互換タイプは準標準仕様「1」を選択してください。\n　その場合、組合せに制限がありますので、組合せ注意事項を\n　参照してください。"]
[null,null,"IS10M-30-D","AC30-D"]
[null,null,"IS10M-40-D","AC40-D"]
[null,null,"IS10M-50-D","AC40-06-D"]
[null,null,"IS10M-60-D","AC50-D\nAC60-D"]
[null,"T形ｽﾍﾟｰｻ付圧力ｽｲｯﾁ","IS10T-20-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","カタログに準拠","下向きの取付けはできません。"]
[null,null,"IS10T-30-D","AC30-D"]
[null,null,"IS10T-40-D","AC40-D"]
[null,null,"IS10T-50-D","AC40-06-D"]
[null,null,"IS10T-60-D","AC50-D\nAC60-D"]
[null,"L形配管ｱﾀﾞﾌﾟﾀ付圧力ｽｲｯﾁ","IS10L-20-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","カタログに準拠","下向きの取付けはできません。"]
[null,null,"IS10L-30-D","AC30-D"]
[null,null,"IS10L-40-D","AC40-D"]
[null,null,"IS10L-50-D","AC40-06-D"]
[null,null,"IS10L-60-D","AC50-D\nAC60-D"]
[null,"配管ｱﾀﾞﾌﾟﾀ付圧力ｽｲｯﾁ","IS10E-20-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","カタログに準拠","下向きの取付けはできません。"]
[null,null,"IS10E-30-D","AC30-D"]
[null,null,"IS10E-40-D","AC40-D"]
[null,null,"IS10E-50-D","AC40-06-D"]
[null,null,"IS10E-60-D","AC50-D\nAC60-D"]
[null,"ｴﾝﾄﾞﾌﾟﾚｰﾄ","E200E-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","カタログに準拠"]
[null,null,"E300E-D","AC30-D"]
[null,null,"E400E-D","AC40-D"]
[null,"ﾁｪｯｸ弁","AKM2000-A","AC20-D","ｱﾀｯﾁﾒﾝﾄ","カタログに準拠","下向きは、向き指定欄に「B」を入力してください。"]
[null,null,"AKM3000-A","AC30-D"]
[null,null,"AKM4000-A","AC40-D"]
[]
[]
[]
[null,"その他付属品：圧力計、圧力スイッチ、サイレンサ、カプラ・継手類"]
[null,"品　名","型式","適用AC","種類","選択範囲","注記"]
[null,"圧力計","Gｼﾘｰｽﾞ\nGPｼﾘｰｽﾞ",null,"付属品","カタログに準拠","同時梱包です。"]
[null,"ﾃﾞｼﾞﾀﾙ圧力ｽｲｯﾁ","ISEｼﾘｰｽﾞ\nZSEｼﾘｰｽﾞ",null,"付属品","カタログに準拠","同時梱包です。"]
[null,"ｻｲﾚﾝｻ","AN*ｼﾘｰｽﾞ\n25*ｼﾘｰｽﾞ\nINAｼﾘｰｽﾞ",null,"付属品","カタログに準拠","同時梱包です。"]
[null,"Sｶﾌﾟﾗｰ","KKｼﾘｰｽﾞ",null,"付属品","カタログに準拠","同時梱包です。"]
[null,"ﾜﾝﾀｯﾁ管継手","KQ2*ｼﾘｰｽﾞ",null,"付属品","カタログに準拠","同時梱包です。"]

{"sheet":"AF","index":2,"n_rows":52,"n_cols":17,"rows_kept":52,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,14],[11,9,11,14],[7,1,7,7],[15,1,17,1],[15,2,17,5],[19,1,24,1],[19,2,24,5],[26,1,28,1],[26,2,28,2],[26,4,28,4],[26,5,28,5],[30,1,49,1],[30,2,49,2],[30,4,35,4],[30,5,35,5],[37,4,40,4],[37,5,40,5],[42,4,43,4],[42,5,43,5],[38,6,39,6],[45,4,46,4],[45,5,46,5],[48,4,49,4],[48,5,49,5]]}
["製品対象リストへ戻る"]
["エアフィルタ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つ　ずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)","50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]","[AC50]","[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","－","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","－","－","－"]
[null,null,null,null,null,null,"06","3／4",null,"－","－","－","●","●","－"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１/８",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１/４",null,"－","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","インジケータ","無記号","インジケータなし",null,"●","●","●","－","●","●"]
[null,null,null,null,null,null,"L","目詰まりチェッカ付",null,"●","●","●","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AFM","index":3,"n_rows":51,"n_cols":13,"rows_kept":51,"cut":false,"hidden":false,"merged":[[19,1,23,1],[19,2,23,5],[0,0,0,6],[25,1,27,1],[25,2,27,2],[25,4,27,4],[25,5,27,5],[7,1,7,7],[10,9,10,12],[11,9,11,12],[15,1,17,1],[15,2,17,5],[10,1,13,5],[10,6,13,6],[10,7,13,7],[29,1,48,1],[29,2,48,2],[29,4,34,4],[29,5,34,5],[36,4,39,4],[36,5,39,5],[41,4,42,4],[41,5,42,5],[37,6,38,6],[44,4,45,4],[44,5,45,5],[47,4,48,4],[47,5,48,5]]}
["製品対象リストへ戻る"]
["ミストセパレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１/８",null,"●","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１/４",null,"－","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","インジケータ","無記号","インジケータなし",null,"●","●","●","－"]
[null,null,null,null,null,null,"L","目詰まりチェッカ付",null,"●","●","●","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AFD","index":4,"n_rows":51,"n_cols":13,"rows_kept":51,"cut":false,"hidden":false,"merged":[[37,6,38,6],[44,4,45,4],[44,5,45,5],[47,4,48,4],[47,5,48,5],[41,4,42,4],[41,5,42,5],[29,1,48,1],[29,2,48,2],[29,4,34,4],[29,5,34,5],[36,4,39,4],[36,5,39,5],[15,1,17,1],[15,2,17,5],[25,1,27,1],[25,2,27,2],[25,4,27,4],[25,5,27,5],[19,1,23,1],[19,2,23,5],[0,0,0,6],[10,9,10,12],[11,9,11,12],[10,1,13,5],[10,6,13,6],[10,7,13,7],[7,1,7,7]]}
["製品対象リストへ戻る"]
["マイクロミストセパレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１/８",null,"●","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１/４",null,"－","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","インジケータ","無記号","インジケータなし",null,"●","●","●","－"]
[null,null,null,null,null,null,"L","目詰まりチェッカ付",null,"●","●","●","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AFG","index":5,"n_rows":48,"n_cols":15,"rows_kept":48,"cut":false,"hidden":false,"merged":[[37,6,38,6],[41,4,42,4],[41,5,42,5],[44,4,45,4],[44,5,45,5],[29,1,45,1],[29,2,45,2],[29,4,34,4],[29,5,34,5],[36,4,39,4],[36,5,39,5],[15,1,17,1],[15,2,17,5],[19,1,23,1],[19,2,23,5],[25,1,27,1],[25,2,27,2],[25,4,27,4],[25,5,27,5],[10,9,10,12],[11,9,11,12],[0,15,0,21],[0,0,0,6],[7,1,7,7],[10,1,13,5],[10,6,13,6],[10,7,13,7]]}
["製品対象リストへ戻る"]
["ウォータセパレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","－"]
[null,null,null,null,null,null,"06","3／4",null,"－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１/８",null,"●","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１/４",null,"－","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AR","index":6,"n_rows":56,"n_cols":17,"rows_kept":56,"cut":false,"hidden":false,"merged":[[10,9,10,14],[11,9,11,14],[48,5,49,5],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[15,1,16,1],[15,2,16,5],[18,1,20,1],[18,2,20,5],[22,1,27,1],[22,2,27,5],[51,4,53,4],[51,5,53,5],[29,1,37,1],[29,2,37,2],[29,4,37,4],[29,5,33,5],[34,5,37,5],[39,1,53,1],[39,2,53,2],[39,4,40,4],[39,5,40,5],[42,4,43,4],[42,5,43,5],[45,4,46,4],[45,5,46,5],[48,4,49,4]]}
["製品対象リストへ戻る"]
["レギュレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。\n"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"➊"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)","50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]","[AC50]\n[AC60]","[AC50]\n[AC60]"]
[]
[null,"➋","逆流機能付",null,null,null,"無記号","逆流機能なし",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｋ","逆流機能付き",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➌","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➍","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","●","－"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➎","オプション",null,"a","圧力計","無記号","圧力計なし",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ","角形埋込式圧力計（リミットインジケータ付）",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｇ","丸形圧力計（リミットインジケータ付）",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ライトアングル角形圧力計（リミットインジケータ付）",null,"●","●","●","●","－","－"]
[null,null,null,null,null,null,"Ｍ","丸形圧力計（カラーゾーン付）",null,"●","●","●","●","●","●"]
[null,null,null,null,null,"デジタル\n圧力スイッチ","Ｅ１","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線下取出し",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ２","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線上取出し",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ３","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線下取出し",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ４","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線上取出し",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➏","準標準",null,"b","設定圧力","無記号","０．０５～０．８５ＭＰａ設定",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"１","０．０２～０．２　ＭＰａ設定",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","排気機構","無記号","リリーフタイプ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ノンリリーフタイプ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","ハンドル向き","無記号","ハンドル下向き",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｙ","ハンドル上向き",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板、圧力計の単位表記：ＭＰａ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板、圧力計の単位表記：ｐｓｉ／°Ｆ\nデジタル圧力スイッチ付：単位切換機能付／初期単位ｐｓｉ",null,"○","○","○","○","○","○"]
[null,null,null,null,null,null,"  ＺA 注2)","デジタル圧力スイッチ：単位切換機能付／初期単位ＭＰａ",null,"○","○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) 海外向けのみに適用",null,null,null,null,"○ 制約条件あり：注1）注2）参照\n"]

{"sheet":"AR□M","index":7,"n_rows":56,"n_cols":12,"rows_kept":56,"cut":false,"hidden":false,"merged":[[41,1,52,1],[41,2,52,2],[41,4,42,4],[41,5,42,5],[44,4,45,4],[44,5,45,5],[47,4,48,4],[47,5,48,5],[50,4,52,4],[50,5,52,5],[27,1,29,1],[27,2,29,5],[31,1,39,1],[31,2,39,2],[31,4,39,4],[31,5,35,5],[36,5,39,5],[15,1,16,1],[15,2,16,5],[18,1,20,1],[18,2,20,5],[22,1,25,1],[22,2,25,5],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,11],[11,9,11,11]]}
["製品対象リストへ戻る"]
["モジュラタイプ共通給気形レギュレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～eの各項目毎に１つずつ選択してください。\n"]
[null,"・オプション・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]"]
[]
[null,"➋","逆流機能付",null,null,null,"無記号","逆流機能なし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｋ","逆流機能付き",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➌","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➍","管接続口径",null,null,null,"０１","１／８",null,"●","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","管接続口径",null,null,null,"０１","１／８",null,"●","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"○注1)","●","●"]
[null,null,null,null,null,null,"０３","３／８",null,"－","－","●"]
[]
[null,"❻","オプション",null,"a","圧力計","無記号","圧力計なし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ","角形埋込式圧力計（リミットインジケータ付）",null,"●","●","●"]
[null,null,null,null,null,null,"Ｇ","丸形圧力計（リミットインジケータ付）",null,"●","●","●"]
[null,null,null,null,null,null,"Ｊ","ライトアングル角形圧力計（リミットインジケータ付）",null,"●","●","●"]
[null,null,null,null,null,null,"Ｍ","丸形圧力計（カラーゾーン付）",null,"●","●","●"]
[null,null,null,null,null,"デジタル\n圧力スイッチ","Ｅ１","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線下取出し",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ２","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線上取出し",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ３","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線下取出し",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ４","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線上取出し",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❼","準標準",null,"b","設定圧力","無記号","０．０５～０．８５ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"１","０．０２～０．２　ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","排気機構","無記号","リリーフタイプ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ノンリリーフタイプ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","ハンドル向き","無記号","ハンドル下向き",null,"●","●","●"]
[null,null,null,null,null,null,"Ｙ","ハンドル上向き",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","圧力単位","無記号","製品銘板と圧力計の単位表記：ＭＰａ",null,"●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注2)","製品銘板、注意銘板、圧力計の単位表記：ｐｓｉ／°Ｆ\nデジタル圧力スイッチ付：単位切換機能付／初期単位ｐｓｉ",null,"○","○","○"]
[null,null,null,null,null,null,"  ＺA 注3)","デジタル圧力スイッチ：単位切換機能付／初期単位ＭＰａ",null,"○","○","○"]
[null,null,null,null,"注1) ＩＮ側管接続口径が1/4の場合のみ選択可",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"○ 制約条件あり：注1）注2）注3）参照\n"]
[null,null,null,null,"注3) 海外向けのみに適用"]

{"sheet":"AL","index":8,"n_rows":44,"n_cols":17,"rows_kept":44,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,14],[11,9,11,14],[37,4,38,4],[37,5,38,5],[40,4,41,4],[40,5,41,5],[15,1,17,1],[15,2,17,5],[19,1,24,1],[19,2,24,5],[26,1,41,1],[26,2,41,2],[26,4,31,4],[26,5,31,5],[33,4,35,4],[33,5,35,5]]}
["製品対象リストへ戻る"]
["ルブリケータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～d の各項目毎に１つずつ選択してください。\n"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"➊"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)","50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]","[AC50]\n[AC60}","[AC50]\n[AC60]"]
[]
[null,"➋","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➌","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","●","－"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"a","ケース","無記号","ポリカーボネートケース",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","油排出口","無記号","ドレンコックなし",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"３","ドレンコック付",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"３Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AW","index":9,"n_rows":68,"n_cols":17,"rows_kept":68,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,13],[11,9,11,13],[15,1,16,1],[15,2,16,5],[18,1,20,1],[18,2,20,5],[22,1,27,1],[22,2,27,5],[29,1,40,1],[29,2,40,2],[29,4,31,4],[29,5,31,5],[33,4,40,4],[33,5,36,5],[37,5,40,5],[63,4,65,4],[63,5,65,5],[42,1,65,1],[42,2,65,2],[42,4,43,4],[42,5,43,5],[45,4,50,4],[45,5,50,5],[52,4,55,4],[52,5,55,5],[53,6,54,6],[57,4,58,4],[57,5,58,5],[60,4,61,4],[60,5,61,5]]}
["製品対象リストへ戻る"]
["フィルタレギュレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～h の各項目毎に１つずつ選択してください。\n"]
[null,"・オプション・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"➊"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]","[AC50]\n[AC60]"]
[]
[null,"➋","逆流機能付",null,null,null,"無記号","逆流機能なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｋ","逆流機能付き",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➌","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➍","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"➎","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","圧力計","無記号","圧力計なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ","角形埋込式圧力計（リミットインジケータ付）",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｇ","丸形圧力計（リミットインジケータ付）",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｍ","丸形圧力計（カラーゾーン付）",null,"●","●","●","●","●"]
[null,null,null,null,null,"デジタル\n圧力スイッチ","Ｅ１","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線下取出し",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ２","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線上取出し",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ３","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線下取出し",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ４","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線上取出し",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➏","準標準",null,"c","設定圧力","無記号","０．０５～０．８５ＭＰａ設定",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"１","０．０２～０．２　ＭＰａ設定",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","ケース","無記号","ポリカーボネートケース",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１/８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１/４",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","排気機構","無記号","リリーフタイプ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ノンリリーフタイプ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"g","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"R","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"h","圧力単位","無記号","製品銘板、注意銘板、圧力計の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板、注意銘板、圧力計の単位表記：ｐｓｉ／°Ｆ\nデジタル圧力スイッチ付：単位切換機能付／初期単位ｐｓｉ",null,"○","○","○","○","○"]
[null,null,null,null,null,null,"  ＺA 注2)","デジタル圧力スイッチ：単位切換機能付／初期単位ＭＰａ",null,"○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) 海外向けのみに適用",null,null,null,null,"○ 制約条件あり：注1）注2）参照\n"]

{"sheet":"AWM","index":10,"n_rows":63,"n_cols":15,"rows_kept":63,"cut":false,"hidden":false,"merged":[[10,7,13,7],[10,9,10,11],[11,9,11,11],[15,1,17,1],[15,2,17,5],[19,1,22,1],[19,2,22,5],[0,0,0,6],[10,1,13,5],[10,6,13,6],[24,1,35,1],[24,2,35,2],[24,4,26,4],[24,5,26,5],[28,4,35,4],[28,5,31,5],[32,5,35,5],[58,4,60,4],[58,5,60,5],[37,1,60,1],[37,2,60,2],[37,4,38,4],[37,5,38,5],[40,4,45,4],[40,5,45,5],[47,4,50,4],[47,5,50,5],[48,6,49,6],[52,4,53,4],[52,5,53,5],[55,4,56,4],[55,5,56,5]]}
["製品対象リストへ戻る"]
["ミストセパレータレギュレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～h の各項目毎に１つずつ選択してください。\n"]
[null,"・オプション・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"➊"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","圧力計","無記号","圧力計なし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ","角形埋込式圧力計（リミットインジケータ付）",null,"●","●","●"]
[null,null,null,null,null,null,"Ｇ","丸形圧力計（リミットインジケータ付）",null,"●","●","●"]
[null,null,null,null,null,null,"Ｍ","丸形圧力計（カラーゾーン付）",null,"●","●","●"]
[null,null,null,null,null,"デジタル\n圧力スイッチ","Ｅ１","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線下取出し",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ２","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線上取出し",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ３","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線下取出し",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ４","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線上取出し",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"c","設定圧力","無記号","０．０５～０．８５ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"１","０．０５～０．２　ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","ケース","無記号","ポリカーボネートケース",null,"●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","ドレン排出口","無記号","ドレンコック付",null,"●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１/８",null,"●","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１/４",null,"－","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","排気機構","無記号","リリーフタイプ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ノンリリーフタイプ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"g","流れ方向","無記号","流れ方向：左→右",null,"●","●","●"]
[null,null,null,null,null,null,"R","流れ方向：右→左",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"h","圧力単位","無記号","製品銘板、注意銘板、圧力計の単位表記：ＭＰａ／°Ｃ",null,"●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板、注意銘板、圧力計の単位表記：ｐｓｉ／°Ｆ\nデジタル圧力スイッチ付：単位切換機能付／初期単位ｐｓｉ",null,"○","○","○"]
[null,null,null,null,null,null,"  ＺA 注2)","デジタル圧力スイッチ：単位切換機能付／初期単位ＭＰａ",null,"○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) 海外向けのみに適用",null,null,null,null,"○ 制約条件あり：注1）注2）参照\n"]

{"sheet":"AWD","index":11,"n_rows":63,"n_cols":15,"rows_kept":63,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,11],[11,9,11,11],[15,1,17,1],[15,2,17,5],[19,1,22,1],[19,2,22,5],[24,1,35,1],[24,2,35,2],[24,4,26,4],[24,5,26,5],[28,4,35,4],[28,5,31,5],[58,4,60,4],[58,5,60,5],[32,5,35,5],[37,1,60,1],[37,2,60,2],[37,4,38,4],[37,5,38,5],[40,4,45,4],[40,5,45,5],[47,4,50,4],[47,5,50,5],[48,6,49,6],[52,4,53,4],[52,5,53,5],[55,4,56,4],[55,5,56,5]]}
["製品対象リストへ戻る"]
["マイクロミストセパレータレギュレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～h の各項目毎に１つずつ選択してください。\n"]
[null,"・オプション・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"➊"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","圧力計","無記号","圧力計なし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ","角形埋込式圧力計（リミットインジケータ付）",null,"●","●","●"]
[null,null,null,null,null,null,"Ｇ","丸形圧力計（リミットインジケータ付）",null,"●","●","●"]
[null,null,null,null,null,null,"Ｍ","丸形圧力計（カラーゾーン付）",null,"●","●","●"]
[null,null,null,null,null,"デジタル\n圧力スイッチ","Ｅ１","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線下取出し",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ２","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線上取出し",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ３","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線下取出し",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ４","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線上取出し",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"c","設定圧力","無記号","０．０５～０．８５ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"１","０．０５～０．２　ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","ケース","無記号","ポリカーボネートケース",null,"●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","ドレン排出口","無記号","ドレンコック付",null,"●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１/８",null,"●","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１/４",null,"－","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","排気機構","無記号","リリーフタイプ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ノンリリーフタイプ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"g","流れ方向","無記号","流れ方向：左→右",null,"●","●","●"]
[null,null,null,null,null,null,"R","流れ方向：右→左",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"h","圧力単位","無記号","製品銘板、注意銘板、圧力計の単位表記：ＭＰａ／°Ｃ",null,"●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板、注意銘板、圧力計の単位表記：ｐｓｉ／°Ｆ\nデジタル圧力スイッチ付：単位切換機能付／初期単位ｐｓｉ",null,"○","○","○"]
[null,null,null,null,null,null,"  ＺA 注2)","デジタル圧力スイッチ：単位切換機能付／初期単位ＭＰａ",null,"○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) 海外向けのみに適用",null,null,null,null,"○ 制約条件あり：注1）注2）参照\n"]

{"sheet":"ARG","index":12,"n_rows":45,"n_cols":14,"rows_kept":45,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[32,1,42,1],[32,2,42,2],[35,4,36,4],[15,1,16,1],[15,2,16,5],[18,1,20,1],[18,2,20,5],[22,1,25,1],[22,2,25,5],[27,1,30,2],[10,9,10,11],[11,9,11,11],[27,4,30,4],[41,4,42,4],[41,5,42,5],[35,5,36,5],[38,4,39,4],[38,5,39,5],[27,5,30,5],[32,4,33,4],[32,5,33,5]]}
["製品対象リストへ戻る"]
["圧力計内蔵レギュレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～eの各項目毎に１つずつ選択してください。\n"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"➊"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]"]
[]
[null,"➋","逆流機能付",null,null,null,"無記号","逆流機能なし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｋ","逆流機能付き",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➌","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➍","管接続口径",null,null,null,"０１","１／８",null,"●","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"➎",null,null,"a","圧力計\n取付角度","Ｇ１","０°",null,"●","●","●"]
[null,null,null,null,null,null,"Ｇ２","９０°",null,"●","●","●"]
[null,null,null,null,null,null,"Ｇ３","１８０°",null,"●","●","●"]
[null,null,null,null,null,null,"Ｇ４","２７０°",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➏","準標準",null,"b","設定圧力","無記号","０．０５～０．８５ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"１","０．０２～０．２　ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","排気機構","無記号","リリーフタイプ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ノンリリーフタイプ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","ハンドル向き","無記号","ハンドル下向き",null,"●","●","●"]
[null,null,null,null,null,null,"Ｙ","ハンドル上向き",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","圧力単位","無記号","製品銘板と圧力計の単位表記：ＭＰａ",null,"●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板：ｐｓｉ、圧力計：ＭＰａ／ｐｓｉ併記",null,"○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AWG","index":13,"n_rows":58,"n_cols":15,"rows_kept":58,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[54,4,55,4],[54,5,55,5],[36,1,55,1],[36,2,55,2],[31,5,34,5],[31,1,34,2],[31,4,34,4],[15,1,16,1],[15,2,16,5],[18,1,20,1],[18,2,20,5],[36,4,37,4],[47,6,48,6],[51,4,52,4],[51,5,52,5],[10,9,10,11],[11,9,11,11],[36,5,37,5],[39,4,44,4],[39,5,44,5],[46,4,49,4],[46,5,49,5],[22,1,25,1],[22,2,25,5],[27,1,29,1],[27,2,29,2],[27,4,29,4],[27,5,29,5]]}
["製品対象リストへ戻る"]
["圧力計内蔵フィルタレギュレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～g の各項目毎に１つずつ選択してください。\n"]
[null,"・オプション・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"➊"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]"]
[]
[null,"➋","逆流機能付",null,null,null,"無記号","逆流機能なし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｋ","逆流機能付き",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➌","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➍","管接続口径",null,null,null,"０１","１／８",null,"●","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"➎","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➏",null,null,"b","圧力計\n取付角度","Ｇ１","０°",null,"●","●","●"]
[null,null,null,null,null,null,"Ｇ２","９０°",null,"●","●","●"]
[null,null,null,null,null,null,"Ｇ３","１８０°",null,"●","●","●"]
[null,null,null,null,null,null,"Ｇ４","２７０°",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➐","準標準",null,"c","設定圧力","無記号","０．０５～０．８５ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"１","０．０２～０．２　ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","ケース","無記号","ポリカーボネートケース",null,"●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","ドレン排出口","無記号","ドレンコック付",null,"●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１/８",null,"●","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１/４",null,"－","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","排気機構","無記号","リリーフタイプ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ノンリリーフタイプ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"g","圧力単位","無記号","製品銘板、ケース注意表示、圧力計の単位表記：ＭＰａ",null,"●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板：ｐｓｉ、ケース注意表示：ｐｓｉ／°Ｆ、\n圧力計：ＭＰａ／ｐｓｉ併記",null,"○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"ARP","index":14,"n_rows":50,"n_cols":14,"rows_kept":50,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,11],[11,9,11,11],[15,1,16,1],[15,2,16,5],[18,1,20,1],[18,2,20,5],[22,1,25,1],[22,2,25,5],[45,5,47,5],[42,5,43,5],[27,4,33,4],[27,5,29,5],[30,5,33,5],[35,4,37,4],[35,5,37,5],[39,4,40,4],[39,5,40,5],[42,4,43,4],[27,1,33,1],[27,2,33,2],[35,1,47,1],[35,2,47,2],[45,4,47,4]]}
["製品対象リストへ戻る"]
["直動精密レギュレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～eの各項目毎に１つずつ選択してください。\n"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"➊"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]"]
[]
[null,"➋","逆流機能付",null,null,null,"無記号","逆流機能なし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｋ","逆流機能付き",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➌","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➍","管接続口径",null,null,null,"０１","１／８",null,"●","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"➎","オプション",null,"a","圧力計","無記号","圧力計なし",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ","角形埋込式圧力計（リミットインジケータ付）",null,"●","●","●"]
[null,null,null,null,null,null,"Ｇ","丸形圧力計（リミットインジケータ付）",null,"●","●","●"]
[null,null,null,null,null,"デジタル\n圧力スイッチ","Ｅ１","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線下取出し",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ２","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線上取出し",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ３","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線下取出し",null,"●","●","●"]
[null,null,null,null,null,null,"Ｅ４","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線上取出し",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➏","準標準",null,"b","設定圧力","無記号","０．００５～０．４　ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"１","０．００５～０．２　ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"３","０．００８～０．６　ＭＰａ設定",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","流れ方向","無記号","流れ方向：左→右",null,"●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","ハンドル向き","無記号","ハンドル下向き",null,"●","●","●"]
[null,null,null,null,null,null,"Ｙ","ハンドル上向き",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","圧力単位","無記号","製品銘板、圧力計の単位表記：ＭＰａ",null,"●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板、圧力計の単位表記：ｐｓｉ／°Ｆ\nデジタル圧力スイッチ付：単位切換機能付／初期単位ｐｓｉ",null,"○","○","○"]
[null,null,null,null,null,null,"  ＺA 注2)","デジタル圧力スイッチ：単位切換機能付／初期単位ＭＰａ",null,"○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) 海外向けのみに適用",null,null,null,null,"○ 制約条件あり：注1）注2）参照\n"]

{"sheet":"AV-A","index":15,"n_rows":61,"n_cols":17,"rows_kept":61,"cut":false,"hidden":false,"merged":[[10,8,13,8],[10,10,10,13],[11,10,11,13],[10,1,13,6],[15,1,17,1],[19,1,23,1],[25,4,26,4],[28,4,29,4],[0,0,0,7],[10,7,13,7],[25,1,29,1],[25,2,29,2],[15,2,17,6],[19,2,23,6],[25,5,26,6],[28,5,29,6],[31,5,36,5],[31,6,34,6],[35,6,36,6],[38,1,43,2],[38,5,43,6],[31,1,36,2],[38,4,43,4],[31,4,36,4],[45,5,46,6],[48,1,50,2],[48,5,50,6],[52,1,56,1],[52,2,56,2],[52,4,53,4],[55,4,56,4],[52,5,53,6],[55,5,56,6],[45,4,46,4],[48,4,50,4],[45,1,46,2]]}
["製品対象リストへ戻る"]
["ソフトスタートアップバルブ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～h の各項目毎に１つずつ選択してください。\n"]
[null,"・オプション・準標準記号は、アルファベットの若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,null,"記号","内容",null,"➊"]
[null,null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,null,20,30,40,"50"]
[null,null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,null,"無記号","Ｒc",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径\n1（Ｐ），２（Ａ）",null,null,null,null,"０２","１／４",null,"●","－","－","－"]
[null,null,null,null,null,null,null,"０３","３／８",null,"－","●","－","－"]
[null,null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－"]
[null,null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●"]
[null,null,null,null,null,null,null,"１０","１",null,"－","－","－","●"]
[null,null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","圧力計",null,"無記号","圧力計なし",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"G","丸形圧力計（リミットインジケータ付）",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","サイレンサ",null,"無記号","サイレンサなし",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"S","サイレンサ（内蔵）",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"＋"]
[null,"❺",null,null,"c","コイル\n定格電圧","AC仕様\n(50／60Hz)",1,"ＡＣ１００Ｖ",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"２","ＡＣ２００Ｖ",null,"●","●","●","●"]
[null,null,null,null,null,null,null,3,"ＡＣ１１０Ｖ［ＡＣ１１５Ｖ］",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"４","ＡＣ２２０Ｖ［ＡＣ２３０Ｖ］",null,"●","●","●","●"]
[null,null,null,null,null,null,"DC仕様","５","ＤＣ２４Ｖ",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"６","ＤＣ１２Ｖ",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"＋"]
[null,"❻",null,null,"d","リード線取出し方法",null,"G","グロメット（リード線長さ３００ｍｍ）",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"Ｄ","Ｄタイプ（ＤＩＮ形ターミナル／コネクタ付）",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"Ｙ","Ｙタイプ（ＤＩＮ形ターミナル／コネクタ付）",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"ＤＯ","Ｄタイプ（ＤＩＮ形ターミナル／コネクタなし）",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"ＹＯ","Ｙタイプ（ＤＩＮ形ターミナル／コネクタなし）",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"　K O 注1)","M12コネクタタイプ（ケーブルなし）",null,"○","○","○","○"]
[null,null,null,null,null,null,null,"＋"]
[null,"❼",null,null,"ｅ","ランプ\nサージ電圧保護回路",null,"無記号","なし",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"     Ｚ 注2)","ランプ・サージ電圧保護回路付",null,"○","○","○","○"]
[null,null,null,null,null,null,null,"＋"]
[null,"❽",null,null,"f","マニュアルの種類",null,"無記号","ノンロックプッシュ操作形",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"Ｂ","プッシュターンロック式ドライバ操作形",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"Ｃ","プッシュターンロック式手操作形",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"＋"]
[null,"❾","準標準",null,"g","流れ方向",null,"無記号","流れ方向：左→右",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"＋"]
[null,null,null,null,"h","圧力単位",null,"無記号","製品銘板と圧力計の単位表記：ＭＰａ",null,"●","●","●","●"]
[null,null,null,null,null,null,null,"     Ｚ 注3)","製品銘板と圧力計の単位表記：ｐｓｉ",null,"○","○","○","○"]
[null,null,null,null,"注1) リード線取出し方法KOは、コイル定格電圧がDC仕様（5,6）のみの対応となります",null,null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) リード線取出し方法DO、YOの場合、ランプ・サージ電圧保護回路付の選択はできません",null,null,null,null,null,"○ 制約条件あり：注1）注2）注3）参照"]
[null,null,null,null,"        リード線取出し方法KOの場合、ランプ・サージ電圧保護回路付のみの対応となります"]
[null,null,null,null,"注3) ネジ種類NPTのみに適用"]

{"sheet":"AFF","index":16,"n_rows":53,"n_cols":14,"rows_kept":53,"cut":false,"hidden":false,"merged":[[11,9,11,13],[10,9,10,13],[19,2,24,5],[30,6,31,6],[49,4,50,4],[49,5,50,5],[39,6,40,6],[46,4,47,4],[46,5,47,5],[10,7,13,7],[43,4,44,4],[43,5,44,5],[30,1,50,1],[30,2,50,2],[38,4,41,4],[38,5,41,5],[30,4,36,4],[30,5,36,5],[26,1,28,1],[26,2,28,2],[26,4,28,4],[26,5,28,5],[19,1,24,1],[0,0,0,6],[15,1,17,1],[15,2,17,5],[10,1,13,5],[10,6,13,6],[7,1,7,7]]}
["製品対象リストへ戻る"]
["ラインフィルタ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC50]","[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","－"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,null,"SUSケース",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１／４",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","インジケータ","無記号","インジケータなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","目詰まりチェッカ付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AM","index":17,"n_rows":53,"n_cols":14,"rows_kept":53,"cut":false,"hidden":false,"merged":[[10,9,10,13],[11,9,11,13],[19,2,24,5],[30,6,31,6],[49,4,50,4],[49,5,50,5],[39,6,40,6],[46,4,47,4],[46,5,47,5],[10,7,13,7],[43,4,44,4],[43,5,44,5],[30,1,50,1],[30,2,50,2],[30,4,36,4],[30,5,36,5],[38,4,41,4],[38,5,41,5],[26,1,28,1],[26,2,28,2],[26,4,28,4],[26,5,28,5],[19,1,24,1],[0,0,0,6],[15,1,17,1],[15,2,17,5],[10,1,13,5],[10,6,13,6]]}
["製品対象リストへ戻る"]
["ミストセパレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC50]","[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","－"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,null,"SUSケース",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１／４",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","インジケータ","無記号","インジケータなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","目詰まりチェッカ付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AMD","index":18,"n_rows":53,"n_cols":14,"rows_kept":53,"cut":false,"hidden":false,"merged":[[10,9,10,13],[11,9,11,13],[19,2,24,5],[30,6,31,6],[49,4,50,4],[49,5,50,5],[39,6,40,6],[46,4,47,4],[46,5,47,5],[10,7,13,7],[43,4,44,4],[43,5,44,5],[30,1,50,1],[30,2,50,2],[30,4,36,4],[30,5,36,5],[38,4,41,4],[38,5,41,5],[26,1,28,1],[26,2,28,2],[26,4,28,4],[26,5,28,5],[19,1,24,1],[0,0,0,6],[15,1,17,1],[15,2,17,5],[10,1,13,5],[10,6,13,6]]}
["製品対象リストへ戻る"]
["マイクロミストセパレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC50]","[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","－"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,null,"SUSケース",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１／４",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","インジケータ","無記号","インジケータなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","目詰まりチェッカ付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"IDG","index":19,"n_rows":39,"n_cols":12,"rows_kept":39,"cut":false,"hidden":false,"merged":[[10,9,10,11],[11,9,11,11],[19,1,22,1],[19,2,22,5],[24,1,31,1],[24,2,31,2],[24,4,25,4],[24,5,25,5],[27,4,28,4],[27,5,28,5],[30,4,31,4],[30,5,31,5],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[15,1,17,1],[15,2,17,5]]}
["製品対象リストへ戻る"]
["メンブレンエアドライヤ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～cの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"a","パージ排出継手","無記号","継手なし",null,"●","●","●"]
[null,null,null,null,null,null,"P　注1)","ワンタッチ管継手付",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","流れ方向","無記号","流れ方向：左→右",null,"●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","圧力単位","無記号","製品銘板の単位表記：ＭＰａ",null,"●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注2)","製品銘板の単位表記：ｐｓｉ",null,"○","○","○"]
[null,null,null,null,"注1) ワンタッチ管継手は、同時梱包となり製品に取付けられていません。",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"○ 制約条件あり：注2）参照\n"]
[]
[]
[null,"組合せ注意事項"]
[null,"本製品の上流側には必ずミストセパレータ(AFM、AM、AWMのいずれか)とマイクロミストセパレータ(AFD、AMD、AWDのいずれか)を取付けてください。"]
[null,"また、供給空気にゴミ(固形異物)が多い場合は、上記の上流側にエアフィルタまたはラインフィルタを取付けてください。"]

{"sheet":"AMK","index":20,"n_rows":40,"n_cols":14,"rows_kept":40,"cut":false,"hidden":false,"merged":[[26,6,27,6],[36,4,37,4],[36,5,37,5],[15,1,17,1],[15,2,17,5],[26,1,37,1],[26,2,37,2],[26,4,31,4],[26,5,31,5],[33,4,34,4],[33,5,34,5],[19,1,24,1],[19,2,24,5],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,13],[11,9,11,13]]}
["製品対象リストへ戻る"]
["活性炭フィルタ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～cの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC50]","[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","－"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"a","ケース","無記号","ポリカーボネートケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,null,"SUSケース",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"PF3A7","index":21,"n_rows":36,"n_cols":16,"rows_kept":36,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,13],[11,9,11,13],[30,1,31,1],[30,2,31,5],[33,1,34,1],[33,2,34,5],[15,1,21,1],[15,2,21,5],[23,1,25,1],[23,2,25,5],[27,1,28,1],[27,2,28,5]]}
["製品対象リストへ戻る"]
["デジタルフロースイッチ"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,"R5","01","02","04","08"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC50]\n[AC60]","[AC50]\n[AC60]"]
[]
[null,"❷","出力仕様",null,null,null,"CS","NPN、アナログ電圧⇔外部入力",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"DS","NPN、アナログ電流⇔外部入力",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"ES","PNP、アナログ電圧⇔外部入力",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"FS","PNP、アナログ電流⇔外部入力",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","IO-Link/スイッチ出力(N/P)",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L3","IO-Link/スイッチ出力(N/P)、アナログ電圧⇔外部入力",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L4","IO-Link/スイッチ出力(N/P)、アナログ電流⇔外部入力",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","オプション",null,null,null,"無記号","M12コネクタ付リード線付(3m)",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"N","M12コネクタ付リード線なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Q","M12-M12コネクタ付リード線付(3m)",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","単位仕様",null,null,null,"無記号注1)","単位切替機能付",null,"○","○","○","○","○"]
[null,null,null,null,null,null,"Ｍ","SI単位固定",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","校正証明書",null,null,null,"無記号","校正証明書なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"A","校正証明書付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❻","流れ方向",null,null,null,"無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"R","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,"注1) 海外向けのみに適用",null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"PF3A8","index":22,"n_rows":30,"n_cols":16,"rows_kept":30,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,13],[11,9,11,13],[27,1,28,1],[27,2,28,5],[15,2,15,5],[17,1,19,1],[17,2,19,5],[21,1,22,1],[21,2,22,5],[24,1,25,1],[24,2,25,5]]}
["製品対象リストへ戻る"]
["圧力/温度付デジタルフロースイッチ"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,"R5","01","02","04","08"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC50]\n[AC60]","[AC50]\n[AC60]"]
[]
[null,"❷","出力仕様",null,null,null,"L2","IO-Link/スイッチ出力(N/P)、スイッチ出力(N/P)",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","オプション",null,null,null,"無記号","M12コネクタ付リード線付(3m)",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"N","M12コネクタ付リード線なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Q","M12-M12コネクタ付リード線付(3m)",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","単位仕様",null,null,null,"無記号注1)","単位切替機能付",null,"○","○","○","○","○"]
[null,null,null,null,null,null,"Ｍ","SI単位固定",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","校正証明書",null,null,null,"無記号","校正証明書なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"A","校正証明書付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❻","流れ方向",null,null,null,"無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"R","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,"注1) 海外向けのみに適用",null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"VP☐E","index":23,"n_rows":39,"n_cols":16,"rows_kept":39,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,8],[10,10,10,13],[11,10,11,13],[15,1,16,1],[15,2,16,5],[15,7,15,8],[16,7,16,8],[18,2,18,5],[18,7,18,8],[20,1,26,1],[20,2,26,5],[20,7,20,8],[21,7,21,8],[22,7,22,8],[23,7,23,8],[24,7,24,8],[25,7,25,8],[26,7,26,8],[35,1,36,1],[35,2,36,5],[35,7,35,8],[36,7,36,8],[28,1,30,1],[28,2,30,5],[28,7,28,8],[29,7,29,8],[30,7,30,8],[32,1,33,1],[32,2,33,5],[32,7,32,8],[33,7,33,8]]}
["製品対象リストへ戻る"]
["3ポート残圧排気弁モジュラ接続タイプ（主弁位置検出機能なし）"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,null,"❶"]
[null,null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,null,"3","5","7","9"]
[null,null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC50]\n[AC60]"]
[]
[null,"❷","圧力仕様",null,null,null,"無記号","標準タイプ(0.2～0.7MPa)",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"K","高圧タイプ(0.2～1.0MPa)",null,null,"－","●","●","－"]
[]
[null,"❸","定格電圧",null,null,null,5,"DC24V",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➍","リード線取出し方法",null,null,null,"D","DIN形ターミナル",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"DO","DIN形ターミナル／コネクタなし",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"DZ","DIN形ターミナル／ランプ・サージ電圧保護回路付",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"Y","DIN(EN175301-803C)形ターミナル",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"YO","DIN(EN175301-803C)形ターミナル／コネクタなし",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"YZ","DIN(EN175301-803C)形ターミナル／ランプ・サージ電圧保護回路付",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"KOZ","M12コネクタ（ケーブルなし）／ランプ・サージ電圧保護回路付",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➎","マニュアル",null,null,null,"無記号","ノンロックプッシュ式",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"A","ノンロックプッシュ式（手操作形）",null,null,"－","●","●","－"]
[null,null,null,null,null,null,"E","プッシュターンロック式（手操作形）",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➏","流れ方向",null,null,null,"無記号","左→右",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"R","右→左",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❼","ソフトスタートアップ機能",null,null,null,"無記号","なし",null,null,"●","●","●","●"]
[null,null,null,null,null,null,"S","ソフトスタートアップ機能付",null,null,"●","●","●","●"]
[null,null,null,null,null,null,null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,null,"○ 制約条件あり\n"]

{"sheet":"VP□R","index":24,"n_rows":41,"n_cols":14,"rows_kept":41,"cut":false,"hidden":false,"merged":[[33,1,34,1],[33,2,34,5],[33,7,33,8],[34,7,34,8],[27,1,28,1],[27,2,28,5],[27,7,27,8],[28,7,28,8],[30,1,31,1],[30,2,31,5],[30,7,30,8],[31,7,31,8],[20,1,21,1],[20,2,21,5],[20,7,20,8],[21,7,21,8],[23,1,25,1],[23,2,25,5],[23,7,23,8],[24,7,24,8],[25,7,25,8],[15,1,16,1],[15,2,16,5],[15,7,15,8],[16,7,16,8],[18,2,18,5],[18,7,18,8],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,8],[10,10,10,11],[11,10,11,11],[36,1,38,1],[36,2,38,5],[36,7,36,8],[38,7,38,8],[37,7,37,8]]}
["製品対象リストへ戻る"]
["主弁位置検出機能付3ポート残圧排気弁モジュラ接続タイプ"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,null,"❶"]
[null,null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,"\n"]
[null,null,null,null,null,null,null,null,null,null,"5","7"]
[null,null,null,null,null,null,null,null,null,null,"[AC30]","[AC40]"]
[]
[null,"❷","弁形式",null,null,null,"無記号","内部パイロット",null,null,"●","●"]
[null,null,null,null,null,null,"R","外部パイロット",null,null,"●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","定格電圧",null,null,null,5,"DC24V",null,null,"●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","リード線取出し方法",null,null,null,"DZ","DIN形ターミナル／ランプ・サージ保護回路付",null,null,"●","●"]
[null,null,null,null,null,null,"YZ","DIN(EN175301-803C)形ターミナル／ランプ・サージ保護回路付",null,null,"●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","セーフティリミットスイッチ\n種類および配線仕様",null,null,null,"無記号","G1/2（オムロン製）",null,null,"●","●"]
[null,null,null,null,null,null,"M","M12コネクタ（オムロン製）",null,null,"●","●"]
[null,null,null,null,null,null,"S1","M12コネクタ（Rockwell Automation製）",null,null,"●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❻","流れ方向",null,null,null,"無記号","左→右",null,null,"●","●"]
[null,null,null,null,null,null,"R","右→左",null,null,"●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❼","残圧排気弁数",null,null,null,"S","シングル",null,null,"●","●"]
[null,null,null,null,null,null,"D","デュアル",null,null,"●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❽","ソフトスタートアップ機能",null,null,null,"無記号","なし",null,null,"●","●"]
[null,null,null,null,null,null,"S","ソフトスタートアップ機能付",null,null,"●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➒","ネジの種類\n(外部パイロットのみ）",null,null,null,"無記号","Rc",null,null,"●","●"]
[null,null,null,null,null,null,"Ｆ","G",null,null,"●","●"]
[null,null,null,null,null,null,"Ｎ","NPT",null,null,"●","●"]
[null,null,null,null,null,null,null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,null,"○ 制約条件あり\n"]

{"sheet":"JSXM","index":25,"n_rows":64,"n_cols":15,"rows_kept":64,"cut":false,"hidden":false,"merged":[[10,10,10,12],[11,10,11,12],[15,2,15,5],[15,7,15,8],[17,2,17,5],[17,7,17,8],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,8],[19,1,20,1],[19,2,20,5],[19,7,19,8],[20,7,20,8],[22,1,26,1],[22,2,26,5],[22,7,23,7],[24,7,26,7],[28,1,30,1],[28,2,30,5],[28,7,28,8],[29,7,29,8],[30,7,30,8],[46,7,46,8],[47,7,47,8],[49,7,49,8],[32,7,32,8],[33,7,33,8],[34,7,34,8],[35,7,35,8],[40,7,40,8],[43,7,43,8],[44,7,44,8],[45,7,45,8],[41,7,41,8],[36,7,36,8],[37,7,37,8],[38,7,38,8],[39,7,39,8],[32,1,41,1],[32,2,41,4],[32,5,39,5],[40,5,41,5],[51,1,52,1],[51,2,52,5],[43,1,49,1],[43,2,49,5],[59,1,60,1],[59,2,60,5],[59,7,59,8],[60,7,60,8],[48,7,48,8],[54,1,57,1],[54,2,57,5],[54,7,54,8],[57,7,57,8],[51,7,51,8],[52,7,52,8],[54,6,55,6],[55,7,55,8],[56,6,57,6],[56,7,56,8]]}
["製品対象リストへ戻る"]
["モジュラー取付形 2ポートソレノイドバルブ"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,null,"❶"]
[null,null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,null,"2","3","4"]
[null,null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]"]
[]
[null,"❷","弁形式",null,null,null,1,"N.C.(ノーマルクローズ）",null,null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","ボディ材質",null,null,null,"A","アルミ",null,null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","シール材質",null,null,null,"Ｎ","NBR",null,null,"●","●","●"]
[null,null,null,null,null,null,"F","FKM",null,null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","オリフィスサイズと管接続口径",null,null,null,"301","オリフィス径：Φ3.2mm","管接続口径：１／8",null,"●","－","－"]
[null,null,null,null,null,null,"302",null,"管接続口径：１／4",null,"●","－","－"]
[null,null,null,null,null,null,"402","オリフィス径：Φ4mm","管接続口径：１／4",null,"－","●","●"]
[null,null,null,null,null,null,"403",null,"管接続口径：３／８",null,"－","●","●"]
[null,null,null,null,null,null,"404",null,"管接続口径：１／2",null,"－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❻","ねじ種類",null,null,null,"R","Rc",null,null,"●","●","●"]
[null,null,null,null,null,null,"N","NPT",null,null,"●","●","●"]
[null,null,null,null,null,null,"F","G",null,null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❼","定格電圧",null,null,"AC仕様",1,"AC100V",null,null,"●","●","●"]
[null,null,null,null,null,null,2,"AC200V",null,null,"●","●","●"]
[null,null,null,null,null,null,3,"AC120(110)V",null,null,"●","●","●"]
[null,null,null,null,null,null,4,"AC220V",null,null,"●","●","●"]
[null,null,null,null,null,null,7,"AC240V",null,null,"●","●","●"]
[null,null,null,null,null,null,8,"AC48V",null,null,"●","●","●"]
[null,null,null,null,null,null,"B","AC24V",null,null,"●","●","●"]
[null,null,null,null,null,null,"J","AC230V",null,null,"●","●","●"]
[null,null,null,null,null,"DC仕様",5,"DC24V",null,null,"●","●","●"]
[null,null,null,null,null,null,6,"DC12V",null,null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❽","リード線取出方法※3",null,null,null,"G","グロメット※1",null,null,"○","○","○"]
[null,null,null,null,null,null,"GS","基板付グロメット（サージ電圧保護回路付）",null,null,"●","●","●"]
[null,null,null,null,null,null,"CS","コンジット（サージ電圧保護回路付）",null,null,"●","●","●"]
[null,null,null,null,null,null,"DS","DIN形ターミナル（サージ電圧保護回路付）",null,null,"●","●","●"]
[null,null,null,null,null,null,"DZ","DIN形ターミナル・ランプ付（サージ電圧保護回路付）",null,null,"●","●","●"]
[null,null,null,null,null,null,"DN","DIN形ターミナル・コネクタ無し（サージ電圧保護回路付）",null,null,"●","●","●"]
[null,null,null,null,null,null,"WN","M12コネクタ・ケーブルなし（サージ電圧保護回路付）※2",null,null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❾","コイル向き",null,null,null,"無記号","上向き",null,null,"●","●","●"]
[null,null,null,null,null,null,"U","下向き",null,null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❿","ブローポート位置",null,null,null,"無記号","コイル上向き：底面（コイル面と反対）",null,null,"●","●","●"]
[null,null,null,null,null,null,null,"コイル下向き：上面（コイル面と反対）",null,null,"●","●","●"]
[null,null,null,null,null,null,"F","コイル上向き：前面",null,null,"●","●","●"]
[null,null,null,null,null,null,null,"コイル下向き：前面",null,null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"⓫","禁油オプション",null,null,null,"無記号","なし",null,null,"●","●","●"]
[null,null,null,null,null,null,"D","禁油",null,null,"●","●","●"]
[null,"※1","DC電圧のみ",null,null,null,null,null,null,null,"● 制約条件なし\n"]
[null,"※2","M12コネクタ用ケーブルは付属されません。",null,null,null,null,null,null,null,"○ 制約条件あり\n"]
[null,"※3","各リード線取出方法のCE対応電圧については、別途カタログを参照ください。"]

{"sheet":"VPX","index":26,"n_rows":77,"n_cols":15,"rows_kept":77,"cut":false,"hidden":false,"merged":[[24,7,24,8],[24,10,24,11],[25,7,25,8],[25,10,25,11],[0,0,0,6],[10,1,14,5],[10,6,14,6],[10,7,14,8],[16,7,16,8],[16,10,16,11],[19,7,19,8],[19,10,19,11],[10,10,11,15],[12,10,12,15],[14,10,14,11],[14,12,14,13],[14,14,14,15],[16,12,16,13],[16,14,16,15],[19,12,19,13],[19,14,19,15],[13,10,13,11],[13,12,13,13],[13,14,13,15],[42,7,42,8],[42,10,42,11],[26,14,26,15],[26,12,26,13],[42,12,42,13],[41,10,41,11],[41,12,41,13],[38,14,38,15],[36,14,36,15],[29,7,29,8],[29,10,29,11],[29,12,29,13],[30,7,30,8],[30,10,30,11],[30,12,30,13],[41,7,41,8],[38,7,38,8],[38,10,38,11],[38,12,38,13],[36,7,36,8],[36,10,36,11],[36,12,36,13],[37,7,37,8],[37,10,37,11],[42,14,42,15],[25,12,25,13],[24,14,24,15],[25,14,25,15],[41,14,41,15],[37,12,37,13],[37,14,37,15],[32,12,32,13],[21,14,21,15],[24,12,24,13],[33,14,33,15],[34,14,34,15],[28,14,28,15],[29,14,29,15],[30,14,30,15],[32,14,32,15],[33,12,33,13],[16,1,17,1],[16,2,17,5],[17,7,17,8],[17,10,17,11],[17,12,17,13],[17,14,17,15],[19,2,19,5],[21,1,22,1],[21,2,22,5],[22,7,22,8],[22,10,22,11],[22,12,22,13],[22,14,22,15],[21,7,21,8],[21,10,21,11],[21,12,21,13],[28,1,30,1],[28,2,30,5],[32,1,39,1],[32,2,39,5],[35,7,35,8],[35,10,35,11],[35,12,35,13],[35,14,35,15],[39,7,39,8],[39,10,39,11],[39,12,39,13],[39,14,39,15],[28,7,28,8],[28,10,28,11],[28,12,28,13],[34,10,34,11],[34,12,34,13],[31,12,31,13],[32,7,32,8],[32,10,32,11],[33,7,33,8],[33,10,33,11],[34,7,34,8],[24,1,26,1],[24,2,26,5],[26,7,26,8],[26,10,26,11],[43,14,43,15],[45,1,47,1],[45,2,47,5],[45,7,45,8],[45,10,45,11],[45,12,45,13],[45,14,45,15],[46,7,46,8],[46,10,46,11],[46,12,46,13],[46,14,46,15],[47,7,47,8],[47,10,47,11],[47,12,47,13],[47,14,47,15],[41,1,43,1],[41,2,43,5],[43,7,43,8],[43,10,43,11],[43,12,43,13]]}
["製品対象リストへ戻る"]
["安全排気バルブ モジュラ接続タイプ"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,null,"❽"]
[]
[null,null,null,null,null,null,null,null,null,null,"適用ACサイズ"]
[null,null,null,null,null,null,null,null,null,null,"A3",null,"A4",null,"A6"]
[null,null,null,null,null,null,null,null,null,null,"[AC30]",null,"[AC40]",null,"[AC50]\n[AC60]"]
[]
[null,"❶","圧力仕様",null,null,null,"無記号","標準(0.25～0.7MPa)",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"K","高圧(0.25～1.0MPa)",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"＋"]
[null,"❷","定格電圧",null,null,null,5,"DC24V",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","リード線取出し方法",null,null,null,"KO","M12コネクタ／コネクタケーブル無し",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"K","M12コネクタ付／ケーブル長さ3000mm",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","ランプ・サージ電圧保護回路\nおよびコモン仕様",null,null,null,"NZ","ランプ・サージ電圧保護回路付／マイナスコモン(CAT.4)",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"D1Z","ランプ・サージ電圧保護回路付／ダブルコモン配線タイプ1(CAT.3)",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"D2Z","ランプ・サージ電圧保護回路付／ダブルコモン配線タイプ2(CAT.3)",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","圧力センサ配線仕様",null,null,null,"D","ダブルコモン",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"N1","マイナスコモン／配線タイプ１",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"N2","マイナスコモン／配線タイプ２",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"＋"]
[null,"❻","圧力計種類",null,null,null,"無記号","圧力計なし",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"G","丸形圧力計(リミットインジケータ付)",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"M","丸形圧力計(カラーゾーン付)",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"E","角形埋込式圧力計(リミットインジケータ付)",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"E1","出力仕様：NPN出力／リード線取出し仕様：配線下取出し",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"E2","出力仕様：NPN出力／リード線取出し仕様：配線上取出し",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"E3","出力仕様：PNP出力／リード線取出し仕様：配線下取出し",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"E4","出力仕様：PNP出力／リード線取出し仕様：配線上取出し",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"＋"]
[null,"❼","圧力計単位表記",null,null,null,"無記号","圧力計単位表記：MPa",null,null,"●",null,"●",null,"●"]
[null,null,null,null,null,null,"  Ｚ 注1)","圧力計単位表記：psi（MPa併記）\nデジタル圧力スイッチ：単位切換機能付／初期単位psi",null,null,"○",null,"○",null,"○"]
[null,null,null,null,null,null,"  ＺA 注1)","デジタル圧力スイッチ：単位切換機能付／初期単位MPa",null,null,"○",null,"○",null,"○"]
[null,null,null,null,null,null,"＋"]
[null,"❾","ねじの種類 注2)\n圧力計接続ねじ[1/8\"]",null,null,null,"無記号","Rc",null,null,"○",null,"○",null,"○"]
[null,null,null,null,null,null,"N","NPT",null,null,"○",null,"○",null,"○"]
[null,null,null,null,null,null,"F","G",null,null,"○",null,"○",null,"○"]
[]
[null,null,"注1) 海外向けのみに適用",null,null,null,null,null,null,null,"● 制約条件なし\n"]
[null,null,"注2) 圧力計種類：無記号, G, M選択時のみねじが切られています。",null,null,null,null,null,null,null,"○ 制約条件あり：注1）注2）参照\n"]
[null,null,"　　　 圧力計種類：Gで圧力計単位表記：Zの場合は、N(NPT)のみ適用"]
[null,null,"注3) サイレンサが必要な場合は、INA-25-100を選定ください。"]
[]
[null,"組合せ注意事項"]
[null,"組合せについて、以下の注意が必要です。"]
[]
[null,"　　①モーメント・振動・衝撃の影響を考慮し、安全排気バルブの両端にはブラケット付スペーサを推奨致します。"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"　　②ALシリーズとの組み合わせはできません。"]

{"sheet":"Y□(T)","index":27,"n_rows":59,"n_cols":16,"rows_kept":59,"cut":false,"hidden":false,"merged":[[20,1,21,1],[20,4,21,5],[20,2,21,2],[17,1,18,1],[17,2,18,5],[0,0,0,6],[12,1,15,5],[12,6,15,6],[12,7,15,7],[12,9,12,13],[13,9,13,13]]}
["製品対象リストへ戻る"]
["スペーサ・ブラケット付スペーサ"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,"200","300","400","500","600"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","スペーサ",null,null,null,"無記号","スペーサ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"T","ブラケット付スペーサ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","準標準",null,"ブラケットタイプ",null,"無記号","標準",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"1","ロングタイプ",null,"○","○","○","－","－"]
[null,null,null,null,"注1) ❷ブラケットでブラケット付スペーサを選択した場合のみ対象となります。",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]
[]
[]
[null,"組合せ注意事項①"]
[null,"モジュラタイプ共通給気形レギュレータの両側にブラケット付スペーサを接続する場合、以下の注意が必要です。"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"組合せ注意事項②"]
[null,"ブラケット付スペーサ・スペーサの配置について、以下の注意が必要です。"]

{"sheet":"VHS","index":28,"n_rows":49,"n_cols":16,"rows_kept":49,"cut":false,"hidden":false,"merged":[[32,1,42,1],[32,2,42,2],[0,0,0,6],[10,1,13,5],[10,6,13,6],[18,1,20,1],[18,2,20,5],[22,1,27,1],[22,2,27,5],[38,4,39,4],[38,5,39,5],[29,1,30,1],[35,4,36,4],[35,5,36,5],[41,4,42,4],[41,5,42,5],[10,7,13,7],[10,9,10,13],[11,9,11,13],[15,1,16,1],[15,2,16,5],[29,2,30,2],[29,4,30,4],[29,5,30,5],[32,4,33,4],[32,5,33,5],[46,1,46,5],[46,6,46,7],[45,9,45,13],[45,1,45,5],[45,6,45,7]]}
["製品対象リストへ戻る"]
["残圧抜き3ポート弁"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～e の各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、アルファベットの若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)","50"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ハンドル操作",null,null,null,"無記号","シングルアクション",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"W","ダブルアクション",null,"●","●","●","●","●"]
[]
[null,"❸","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","管接続口径",null,null,null,"01","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","－","－"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","オプション",null,"a","サイレンサ","無記号","なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"S","内蔵式サイレンサ付（EXHポート用）",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❻","準標準",null,"b","ハンドル色","無記号","赤",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｋ","黒",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ハンドル材質","無記号","樹脂",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｍ","金属",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","圧力単位","無記号","製品銘板の単位表記：ＭＰａ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板の単位表記：ｐｓｉ",null,"○","○","○","○","○"]
[]
[null,"オーダーメイド"]
[null,"記号",null,null,null,null,"内容"]
[null,"X1",null,null,null,null,"ボディ赤色+難燃仕様",null,null,"●","●","●","●","●"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"E□00","index":29,"n_rows":26,"n_cols":14,"rows_kept":26,"cut":false,"hidden":false,"merged":[[0,0,0,6],[9,9,9,13],[10,9,10,13],[14,1,16,1],[14,2,16,5],[18,1,25,1],[18,2,25,5],[9,1,12,5],[9,6,12,6],[9,7,12,7]]}
["製品対象リストへ戻る"]
["配管アダプタ"]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"200","300","400","500","600"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"12","１　１／４",null,"－","－","－","－","●"]
[null,null,null,null,null,null,"14","１　１／２",null,"－","－","－","－","●"]

{"sheet":"E□00L","index":30,"n_rows":25,"n_cols":14,"rows_kept":25,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,9,10,13],[11,9,11,13],[15,1,17,1],[15,2,17,5],[19,1,24,1],[19,2,24,5],[10,1,13,5],[10,6,13,6],[10,7,13,7]]}
["製品対象リストへ戻る"]
["L形配管アダプタ"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"200","300","400","500","600"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","－","●"]

{"sheet":"E□00T","index":31,"n_rows":25,"n_cols":14,"rows_kept":25,"cut":false,"hidden":false,"merged":[[19,1,24,1],[19,2,24,5],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,13],[11,9,11,13],[15,1,17,1],[15,2,17,5]]}
["製品対象リストへ戻る"]
["T形配管アダプタ"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"200","300","400","500","600"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","－","●"]

{"sheet":"Y□10","index":32,"n_rows":92,"n_cols":14,"rows_kept":92,"cut":false,"hidden":false,"merged":[[32,9,32,13],[0,0,0,6],[15,9,15,13],[16,9,16,13],[24,1,28,1],[24,2,28,5],[15,1,18,5],[15,6,18,6],[15,7,18,7],[30,1,31,1],[30,2,31,2],[30,4,31,5],[20,1,22,1],[20,2,22,5]]}
["製品対象リストへ戻る"]
["T形スペーサ"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"210","310","410","510","610"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","●","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","○","●","●","●"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","○","○","●"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","○","○"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"ボディタイプ",null,"無記号","標準",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"1","薄形",null,"●","●","●","●","●"]
[null,null,null,null,null,null,null,null,null,"● 制約条件なし"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：❹ボディタイプ「標準」のみ"]
[]
[]
[null,"組合せ注意事項"]
[null,"上記品番体系で、準標準仕様「1」を選択すると、従来品と面間寸法に互換性のある製品となります。"]
[null,"その場合、以下の組合せに注意が必要です。"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"又は"]

{"sheet":"Y□4","index":33,"n_rows":36,"n_cols":14,"rows_kept":36,"cut":false,"hidden":false,"merged":[[0,0,0,6],[17,9,17,13],[18,9,18,13],[26,1,30,1],[26,2,30,5],[17,1,20,5],[17,6,20,6],[17,7,20,7],[34,9,34,13],[32,1,33,1],[32,2,33,2],[32,4,33,5],[22,1,24,1],[22,2,24,5]]}
["製品対象リストへ戻る"]
["クロススペーサ"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"24","34","44","54","64"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","○","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"ボディタイプ",null,"無記号","標準",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"1","前後ポート選択形",null,"●","●","●","●","－"]
[null,null,null,null,null,null,null,null,null,"● 制約条件なし"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：❹ボディタイプ「標準」のみ"]

{"sheet":"IS10M","index":34,"n_rows":98,"n_cols":14,"rows_kept":98,"cut":false,"hidden":false,"merged":[[15,1,26,1],[15,2,26,2],[15,4,16,4],[15,5,16,5],[18,4,20,4],[18,5,20,5],[22,4,23,4],[22,5,23,5],[25,4,26,4],[25,5,26,5],[0,0,0,6],[10,9,10,13],[11,9,11,13],[10,1,13,5],[10,6,13,6],[10,7,13,7]]}
["製品対象リストへ戻る"]
["圧力スイッチ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～d の各項目毎に１つ　ずつ選択してください。\n"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"20","30","40","50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","準標準",null,"a","設定圧力範囲","無記号","0.1~0.4MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"6 注1)","0.1~0.6MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","リード線長さ","無記号","0.5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","3m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Z","5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","目盛板圧力単位","無記号","MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｐ注2)","MPa・psi併記",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","ボディタイプ","無記号","標準",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"1","薄形",null,"●","●","●","●","●"]
[null,null,null,null,"注1) ❷準標準で\"6P\"を選択した場合、設定圧力範囲は0.2～0.6MPa(30～90psi)になります。"]
[null,null,null,null,"注2) 海外向けのみに適用。"]
[]
[]
[null,"組合せ注意事項"]
[null,"上記品番体系で、準標準仕様「1」を選択すると、従来品と面間寸法に互換性のある製品となります。"]
[null,"その場合、以下の組合せに注意が必要です。"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"又は"]

{"sheet":"IS10T","index":35,"n_rows":36,"n_cols":14,"rows_kept":36,"cut":false,"hidden":false,"merged":[[10,9,10,13],[11,9,11,13],[19,1,23,1],[19,2,23,5],[15,1,17,1],[15,2,17,5],[10,7,13,7],[0,0,0,6],[25,1,33,1],[25,2,33,2],[25,4,26,4],[25,5,26,5],[28,4,30,4],[28,5,30,5],[32,4,33,4],[32,5,33,5],[10,1,13,5],[10,6,13,6]]}
["製品対象リストへ戻る"]
["Ｔ形スペーサ付圧力スイッチ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～c の各項目毎に１つ　ずつ選択してください。\n"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"20","30","40","50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","●","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"a","設定圧力範囲","無記号","0.1~0.4MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"6 注1)","0.1~0.6MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","リード線長さ","無記号","0.5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","3m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Z","5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","目盛板圧力単位","無記号","MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｐ注2)","MPa・psi併記",null,"●","●","●","●","●"]
[null,null,null,null,"注1) ❹準標準で\"6P\"を選択した場合、設定圧力範囲は0.2～0.6MPa(30～90psi)になります。"]
[null,null,null,null,"注2) 海外向けのみに適用。"]

{"sheet":"IS10L","index":36,"n_rows":40,"n_cols":14,"rows_kept":40,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,9,10,13],[11,9,11,13],[10,1,13,5],[10,6,13,6],[10,7,13,7],[15,1,17,1],[15,2,17,5],[36,4,37,4],[36,5,37,5],[19,1,24,1],[19,2,24,5],[26,1,37,1],[26,2,37,2],[26,4,27,4],[26,5,27,5],[29,4,31,4],[29,5,31,5],[33,4,34,4],[33,5,34,5]]}
["製品対象リストへ戻る"]
["Ｌ形配管アダプタ付圧力スイッチ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～d の各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"a","設定圧力範囲","無記号","0.1~0.4MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"6 注1)","0.1~0.6MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","リード線長さ","無記号","0.5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","3m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Z","5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","目盛板圧力単位","無記号","MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｐ注2)","MPa・psi併記",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","取付位置","無記号","右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","左",null,"●","●","●","●","●"]
[null,null,null,null,"注1) ❹準標準で\"6P\"を選択した場合、設定圧力範囲は0.2～0.6MPa(30～90psi)になります。"]
[null,null,null,null,"注2) 海外向けのみに適用。"]

{"sheet":"IS10E","index":37,"n_rows":42,"n_cols":14,"rows_kept":42,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,9,10,13],[11,9,11,13],[10,1,13,5],[10,6,13,6],[10,7,13,7],[15,1,17,1],[15,2,17,5],[38,4,39,4],[38,5,39,5],[19,1,26,1],[19,2,26,5],[28,1,39,1],[28,2,39,2],[28,4,29,4],[28,5,29,5],[31,4,33,4],[31,5,33,5],[35,4,36,4],[35,5,36,5]]}
["製品対象リストへ戻る"]
["配管アダプタ付圧力スイッチ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～d の各項目毎に１つ　ずつ選択してください。\n"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"20","30",40,"50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"12","１　１／４",null,"－","－","－","－","●"]
[null,null,null,null,null,null,"14","１　１／２",null,"－","－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"a","設定圧力範囲","無記号","0.1~0.4MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"6 注1)","0.1~0.6MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","リード線長さ","無記号","0.5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","3m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Z","5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","目盛板圧力単位","無記号","MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｐ注2)","MPa・psi併記",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","取付位置","無記号","右端用",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","左端用",null,"●","●","●","●","●"]
[null,null,null,null,"注1) ❹準標準で\"6P\"を選択した場合、設定圧力範囲は0.2～0.6MPa(30～90psi)になります。"]
[null,null,null,null,"注2) 海外向けのみに適用。"]

{"sheet":"E□00E","index":38,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,6],[9,1,10,5],[9,6,10,6],[9,7,10,7],[12,1,14,1],[12,2,14,5]]}
["製品対象リストへ戻る"]
["エンドプレート"]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容"]
[]
[]
[null,"❶","ボディサイズ",null,null,null,200,"AC20-D用"]
[null,null,null,null,null,null,"300","AC30-D用"]
[null,null,null,null,null,null,"400","AC40-D用"]

{"sheet":"AKM","index":39,"n_rows":21,"n_cols":12,"rows_kept":21,"cut":false,"hidden":false,"merged":[[18,1,20,1],[18,2,20,5],[0,0,0,6],[9,1,12,5],[9,6,12,6],[9,7,12,7],[9,9,9,11],[10,9,10,11],[14,1,16,1],[14,2,16,5]]}
["製品対象リストへ戻る"]
["チェック弁"]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"20","30","40"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","分岐ポート\n管接続口径",null,null,null,"01","１／８",null,"●","●","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●"]
[null,null,null,null,null,null,"03","３／８",null,"－","－","●"]