{"text_format":"1","workbook":"xlsx","n_sheets":23,"sheets":["仕様書 ","対象製品ﾘｽﾄ","AF","AFM","AFD","AR","AW","AFF","AM","AMD","AMK","Y□(T)","VHS","E□00","E□00L","E□00T","Y□10","Y□4","IS10M","IS10T","IS10L","IS10E","E□00E"],"not_rendered":{"charts":0,"images":70,"macros":1,"external_links":1,"defined_names":21,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"仕様書 ","index":0,"n_rows":54,"n_cols":50,"rows_kept":54,"cut":false,"hidden":false,"merged":[[52,32,52,33],[52,34,52,37],[52,38,52,39],[52,40,52,43],[52,44,52,46],[52,47,52,49],[51,44,51,46],[51,47,51,49],[52,2,52,5],[52,6,52,7],[52,8,52,11],[52,12,52,13],[52,14,52,17],[52,18,52,20],[52,21,52,23],[52,28,52,31],[51,32,51,33],[51,34,51,35],[51,36,51,37],[51,38,51,39],[51,40,51,41],[51,42,51,43],[51,14,51,15],[51,16,51,17],[51,18,51,20],[51,21,51,23],[51,28,51,29],[51,30,51,31],[51,2,51,3],[51,4,51,5],[51,6,51,7],[51,8,51,9],[51,10,51,11],[51,12,51,13],[46,10,47,14],[46,36,47,40],[49,2,49,5],[49,6,49,23],[49,28,49,31],[49,32,49,49],[43,3,43,10],[43,14,43,22],[43,31,43,38],[43,41,43,47],[44,3,44,10],[44,14,44,22],[44,31,44,38],[44,41,44,47],[41,3,41,10],[41,14,41,22],[41,31,41,38],[41,41,41,47],[42,3,42,10],[42,14,42,22],[42,31,42,38],[42,41,42,47],[39,3,39,10],[39,14,39,22],[39,31,39,38],[39,41,39,47],[40,3,40,10],[40,14,40,22],[40,31,40,38],[40,41,40,47],[36,41,36,47],[37,3,37,10],[37,14,37,22],[37,31,37,38],[37,41,37,47],[38,3,38,10],[38,14,38,22],[38,31,38,38],[38,41,38,47],[34,3,34,10],[34,15,34,22],[34,31,34,38],[35,3,35,10],[35,31,35,38],[36,3,36,10],[36,14,36,22],[36,31,36,38],[32,3,32,10],[32,15,32,22],[32,31,32,38],[33,3,33,10],[33,15,33,22],[33,31,33,38],[30,3,30,10],[30,15,30,22],[30,31,30,38],[31,3,31,10],[31,15,31,22],[31,31,31,38],[28,3,28,10],[28,15,28,22],[28,31,28,38],[29,3,29,10],[29,15,29,22],[29,31,29,38],[26,3,26,10],[26,15,26,22],[26,31,26,38],[27,3,27,10],[27,15,27,22],[27,31,27,38],[23,2,23,4],[23,30,23,32],[24,3,24,10],[24,15,24,22],[24,31,24,38],[25,3,25,10],[25,15,25,22],[25,31,25,38],[4,22,4,23],[5,2,5,4],[5,5,5,9],[5,10,5,12],[5,13,5,16],[5,17,5,19],[5,20,5,23],[4,2,4,4],[4,5,4,9],[4,10,4,12],[4,13,4,16],[4,17,4,19],[4,20,4,21],[0,2,0,4],[0,5,0,23],[2,15,2,16],[2,17,2,18],[3,2,3,4],[3,5,3,9],[3,10,3,12],[3,13,3,16],[3,17,3,19],[3,20,3,23]]}
[null,null,"SMC株式会社",null,null,"F.R.L. エアコンビネーション 組合せ簡易特注品仕様書"]
[null,null,"お客様ご記入欄",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"記入例"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"作成日",null,null,null,"年",null,"月",null,"日"]
[null,null,"貴社名",null,null,null,null,null,null,null,"貴部署名",null,null,null,null,null,null,"ご担当者名"]
[null,null,"ＴＥＬ",null,null,null,null,null,null,null,"ＦＡＸ",null,null,null,null,null,null,"リピート"]
[null,null,"装置名(NO.)",null,null,null,null,null,null,null,"図　番",null,null,null,null,null,null,"工番・作番"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"組合せ表",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"組合せ表"]
[null,null,"組付\n位置","品番記載欄",null,null,null,null,null,null,null,"向き\n指定",null,null,"組付\n位置","品番記載欄",null,null,null,null,null,null,null,"向き\n指定",null,null,null,null,null,null,"組付\n位置","品番記載欄",null,null,null,null,null,null,null,"向き\n指定"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"E300-04-D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"Y300T-D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"HF1B-AF30-03-D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"Y300T-D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"Y310-02-D",null,null,null,null,null,null,null,"B"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"Y300T-D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"HF1B-AR30-03-D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"Y300T-D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"HF1B-VHS30-03-D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"Y300T-D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"同梱製品",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,"E300-04-D",null,null,null,null,null,null,null,null,null,"同梱製品"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"品番記載欄",null,null,null,null,null,null,null,null,"数量",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"品番記載欄",null,null,null,null,null,null,"数量"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"以下SMC担当記入欄",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"以下SMC担当記入欄"]
[]
[null,null,"ご発注品番　(この品番で手配下さるよう、お願い申し上げます。)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ご発注品番　(この品番で手配下さるよう、お願い申し上げます。)"]
[null,null,"簡易特注品番",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"簡易特注品番",null,null,null,"AC＊＊X-＊＊＊＊＊-D"]
[]
[null,null,"客先コード",null,null,null,"U/C",null,null,null,"部署ｺｰﾄﾞ",null,null,null,"担当ｺｰﾄﾞ",null,null,null,"イメージ登録No.",null,null,null,null,null,null,null,null,null,"客先コード",null,null,null,"U/C",null,null,null,"部署ｺｰﾄﾞ",null,null,null,"担当ｺｰﾄﾞ",null,null,null,"イメージ登録No."]
[null,null,"ＦＡＸ手配時記入欄",null,null,null,"客先注番",null,null,null,null,null,"客先納期",null,null,null,null,null,"ＳＭＣ手配Ｎｏ",null,null,null,null,null,null,null,null,null,"ＦＡＸ手配時記入欄",null,null,null,"客先注番",null,null,null,null,null,"客先納期",null,null,null,null,null,"ＳＭＣ手配Ｎｏ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"シリアルNo.HF1B-AC※※X-D_1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"X54","v":"シリアルNo.HF1B-AC※※X-D_1"}]

{"sheet":"対象製品ﾘｽﾄ","index":1,"n_rows":123,"n_cols":7,"rows_kept":123,"cut":false,"hidden":false,"merged":[[62,6,66,6],[39,1,43,1],[39,4,43,4],[39,6,43,6],[34,6,38,6],[62,1,66,1],[39,5,43,5],[62,5,66,5],[44,5,48,5],[44,4,48,4],[57,6,61,6],[62,4,66,4],[52,6,56,6],[44,1,48,1],[45,6,48,6],[107,4,111,4],[72,1,76,1],[67,1,71,1],[77,5,81,5],[72,4,76,4],[72,5,76,5],[67,4,71,4],[67,5,71,5],[77,1,81,1],[34,5,38,5],[34,1,38,1],[67,6,71,6],[107,6,111,6],[97,4,101,4],[97,5,101,5],[97,6,101,6],[82,5,86,5],[82,6,86,6],[72,6,76,6],[77,4,81,4],[77,6,81,6],[87,6,91,6],[82,4,86,4],[92,4,96,4],[92,5,96,5],[97,1,101,1],[4,5,9,5],[4,4,9,4],[4,6,9,6],[4,1,9,1],[10,4,13,4],[10,5,13,5],[10,1,13,1],[10,6,13,6],[29,6,33,6],[18,1,23,1],[52,5,56,5],[29,5,33,5],[29,1,33,1],[29,4,33,4],[34,4,38,4],[82,1,86,1],[112,6,114,6],[102,5,106,5],[102,4,106,4],[102,1,106,1],[92,6,96,6],[102,6,106,6],[92,1,96,1],[107,5,111,5],[112,1,114,1],[112,4,114,4],[112,5,114,5],[87,1,91,1],[87,4,91,4],[87,5,91,5],[107,1,111,1],[14,1,17,1],[14,4,17,4],[14,5,17,5],[14,6,17,6],[57,4,61,4],[57,5,61,5],[52,1,56,1],[52,4,56,4],[57,1,61,1],[18,4,23,4],[18,5,23,5],[18,6,23,6],[24,6,28,6],[24,1,28,1],[24,4,28,4],[24,5,28,5]]}
[null,"対象製品ﾘｽﾄ"]
[]
[null,"FRL-D　対象製品"]
[null,"品　名","型式","適用AC","種　類","選択範囲","注記"]
[null,"ｴｱﾌｨﾙﾀ","HF1B-AF20-D","AC20-D","製品","HF1B-Series カタログに準拠\n（但し、AF用ブラケットは選択できません。）"]
[null,null,"HF1B-AF30-D","AC30-D"]
[null,null,"HF1B-AF40-D","AC40-D"]
[null,null,"HF1B-AF40-06-D","AC40-06-D"]
[null,null,"HF1B-AF50-D","AC50-D\nAC60-D"]
[null,null,"HF1B-AF60-D","AC50-D\nAC60-D"]
[null,"ﾐｽﾄｾﾊﾟﾚｰﾀ","HF1B-AFM20-D","AC20-D","製品","HF1B-Series カタログに準拠\n（但し、AFM用ブラケットは選択できません。）"]
[null,null,"HF1B-AFM30-D","AC30-D"]
[null,null,"HF1B-AFM40-D","AC40-D"]
[null,null,"HF1B-AFM40-06-D","AC40-06-D"]
[null,"ﾏｲｸﾛﾐｽﾄｾﾊﾟﾚｰﾀ","HF1B-AFD20-D","AC20-D","製品","HF1B-Series カタログに準拠\n（但し、AFD用ブラケットは選択できません。）"]
[null,null,"HF1B-AFD30-D","AC30-D"]
[null,null,"HF1B-AFD40-D","AC40-D"]
[null,null,"HF1B-AFD40-06-D","AC40-06-D"]
[null,"ﾚｷﾞｭﾚｰﾀ","HF1B-AR20(K)-D","AC20-D","製品","HF1B-Series カタログに準拠\n（但し、AR用ブラケット、パネルマウント用セットナットは選択できません。）"]
[null,null,"HF1B-AR30(K)-D","AC30-D"]
[null,null,"HF1B-AR40(K)-D","AC40-D"]
[null,null,"HF1B-AR40(K)-06-D","AC40-06-D"]
[null,null,"HF1B-AR50(K)-D","AC50-D\nAC60-D"]
[null,null,"HF1B-AR60(K)-D","AC50-D\nAC60-D"]
[null,"ﾌｨﾙﾀﾚｷﾞｭﾚｰﾀ","HF1B-AW20(K)-D","AC20-D","製品","HF1B-Series カタログに準拠\n（但し、AW用ブラケット、パネルマウント用セットナットは選択できません。）"]
[null,null,"HF1B-AW30(K)-D","AC30-D"]
[null,null,"HF1B-AW40(K)-D","AC40-D"]
[null,null,"HF1B-AW40(K)-06-D","AC40-06-D"]
[null,null,"HF1B-AW60(K)-D","AC50-D\nAC60-D"]
[null,"ﾗｲﾝﾌｨﾙﾀ","HF1B-AFF20-D","AC20-D","製品","HF1B-Series カタログに準拠\n（但し、AFF用ブラケットは選択できません。）"]
[null,null,"HF1B-AFF30-D","AC30-D"]
[null,null,"HF1B-AFF40-D","AC40-D"]
[null,null,"HF1B-AFF50-D","AC50-D"]
[null,null,"HF1B-AFF60-D","AC60-D"]
[null,"ﾐｽﾄｾﾊﾟﾚｰﾀ","HF1B-AM20-D","AC20-D","製品","HF1B-Series カタログに準拠\n（但し、AM用ブラケットは選択できません。）"]
[null,null,"HF1B-AM30-D","AC30-D"]
[null,null,"HF1B-AM40-D","AC40-D"]
[null,null,"HF1B-AM50-D","AC50-D"]
[null,null,"HF1B-AM60-D","AC60-D"]
[null,"ﾏｲｸﾛﾐｽﾄｾﾊﾟﾚｰﾀ","HF1B-AMD20-D","AC20-D","製品","HF1B-Series カタログに準拠\n（但し、AMD用ブラケットは選択できません。）"]
[null,null,"HF1B-AMD30-D","AC30-D"]
[null,null,"HF1B-AMD40-D","AC40-D"]
[null,null,"HF1B-AMD50-D","AC50-D"]
[null,null,"HF1B-AMD60-D","AC60-D"]
[null,"活性炭ﾌｨﾙﾀ","HF1B-AMK20-D","AC20-D","製品","HF1B-Series カタログに準拠\n（但し、AMK用ブラケットは選択できません。）"]
[null,null,"HF1B-AMK30-D","AC30-D"]
[null,null,"HF1B-AMK40-D","AC40-D"]
[null,null,"HF1B-AMK50-D","AC50-D"]
[null,null,"HF1B-AMK60-D","AC60-D"]
[]
[null,"FRL-D スペーサ、アタッチメント"]
[null,"品　名","型式","適用AC","種類","選択範囲","注記"]
[null,"ｽﾍﾟｰｻ","Y200-D","AC20-D","ｽﾍﾟｰｻ","標準カタログに準拠"]
[null,null,"Y300-D","AC30-D"]
[null,null,"Y400-D","AC40-D"]
[null,null,"Y500-D","AC40-06-D"]
[null,null,"Y600-D","AC50-D\nAC60-D"]
[null,"ﾌﾞﾗｹｯﾄ付ｽﾍﾟｰｻ","Y200T-D","AC20-D","ｽﾍﾟｰｻ","標準カタログに準拠"]
[null,null,"Y300T-D","AC30-D"]
[null,null,"Y400T-D","AC40-D"]
[null,null,"Y500T-D","AC40-06-D"]
[null,null,"Y600T-D","AC50-D\nAC60-D"]
[null,"残圧抜き3ﾎﾟｰﾄ弁","HF1B-VHS20-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","HF1B-Series カタログに準拠\n（但し、VHS用ブラケットは選択できません。）"]
[null,null,"HF1B-VHS30-D","AC30-D"]
[null,null,"HF1B-VHS40-D","AC40-D"]
[null,null,"HF1B-VHS40-06-D","AC40-06-D"]
[null,null,"HF1B-VHS50-D","AC50-D\nAC60-D"]
[null,"配管ｱﾀﾞﾌﾟﾀ","E200-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","標準カタログに準拠"]
[null,null,"E300-D","AC30-D"]
[null,null,"E400-D","AC40-D"]
[null,null,"E500-D","AC40-06-D"]
[null,null,"E600-D","AC50-D\nAC60-D"]
[null,"L形配管ｱﾀﾞﾌﾟﾀ","E200L-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","標準カタログに準拠","下向きは、向き指定欄に「B」を入力してください。"]
[null,null,"E300L-D","AC30-D"]
[null,null,"E400L-D","AC40-D"]
[null,null,"E500L-D","AC40-06-D"]
[null,null,"E600L-D","AC50-D\nAC60-D"]
[null,"T形配管ｱﾀﾞﾌﾟﾀ","E200T-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","標準カタログに準拠"]
[null,null,"E300T-D","AC30-D"]
[null,null,"E400T-D","AC40-D"]
[null,null,"E500T-D","AC40-06-D"]
[null,null,"E600T-D","AC50-D\nAC60-D"]
[null,"T形ｽﾍﾟｰｻ","Y210-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","標準カタログに準拠","・下向きは、向き指定欄に「B」を入力してください。\n・従来品と面間互換タイプは準標準仕様「1」を選択してください。\n　その場合、組合せに制限がありますので、組合せ注意事項を\n　参照してください。"]
[null,null,"Y310-D","AC30-D"]
[null,null,"Y410-D","AC40-D"]
[null,null,"Y510-D","AC40-06-D"]
[null,null,"Y610-D","AC50-D\nAC60-D"]
[null,"ｸﾛｽｽﾍﾟｰｻ","Y24-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","標準カタログに準拠","従来品と面間互換タイプは準標準仕様「1」を選択してください。"]
[null,null,"Y34-D","AC30-D"]
[null,null,"Y44-D","AC40-D"]
[null,null,"Y54-D","AC40-06-D"]
[null,null,"Y64-D","AC50-D\nAC60-D"]
[null,"圧力ｽｲｯﾁ","HF1B-IS10M-20-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","HF1B-Series 本データシートに準拠","・下向きの取付けはできません。\n・従来品と面間互換タイプは準標準仕様「1」を選択してください。\n　その場合、組合せに制限がありますので、組合せ注意事項を\n　参照してください。"]
[null,null,"HF1B-IS10M-30-D","AC30-D"]
[null,null,"HF1B-IS10M-40-D","AC40-D"]
[null,null,"HF1B-IS10M-50-D","AC40-06-D"]
[null,null,"HF1B-IS10M-60-D","AC50-D\nAC60-D"]
[null,"T形ｽﾍﾟｰｻ付圧力ｽｲｯﾁ","HF1B-IS10T-20-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","HF1B-Series 本データシートに準拠","下向きの取付けはできません。"]
[null,null,"HF1B-IS10T-30-D","AC30-D"]
[null,null,"HF1B-IS10T-40-D","AC40-D"]
[null,null,"HF1B-IS10T-50-D","AC40-06-D"]
[null,null,"HF1B-IS10T-60-D","AC50-D\nAC60-D"]
[null,"L形配管ｱﾀﾞﾌﾟﾀ付圧力ｽｲｯﾁ","HF1B-IS10L-20-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","HF1B-Series 本データシートに準拠","下向きの取付けはできません。"]
[null,null,"HF1B-IS10L-30-D","AC30-D"]
[null,null,"HF1B-IS10L-40-D","AC40-D"]
[null,null,"HF1B-IS10L-50-D","AC40-06-D"]
[null,null,"HF1B-IS10L-60-D","AC50-D\nAC60-D"]
[null,"配管ｱﾀﾞﾌﾟﾀ付圧力ｽｲｯﾁ","HF1B-IS10E-20-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","HF1B-Series 本データシートに準拠","下向きの取付けはできません。"]
[null,null,"HF1B-IS10E-30-D","AC30-D"]
[null,null,"HF1B-IS10E-40-D","AC40-D"]
[null,null,"HF1B-IS10E-50-D","AC40-06-D"]
[null,null,"HF1B-IS10E-60-D","AC50-D\nAC60-D"]
[null,"ｴﾝﾄﾞﾌﾟﾚｰﾄ","E200E-D","AC20-D","ｱﾀｯﾁﾒﾝﾄ","標準カタログに準拠"]
[null,null,"E300E-D","AC30-D"]
[null,null,"E400E-D","AC40-D"]
[]
[]
[]
[null,"その他付属品：圧力計、圧力スイッチ、継手類"]
[null,"品　名","型式","適用AC","種類","選択範囲","注記"]
[null,"圧力計","Gｼﾘｰｽﾞ\nGAｼﾘｰｽﾞ",null,"付属品","HF1B-Series カタログに準拠","同時梱包です。"]
[null,"ﾃﾞｼﾞﾀﾙ圧力ｽｲｯﾁ","ISEｼﾘｰｽﾞ\nZSEｼﾘｰｽﾞ",null,"付属品","HF1B-Series カタログに準拠","同時梱包です。"]
[null,"管継手","KFｼﾘｰｽﾞ\nM, MSｼﾘｰｽﾞ\nH/DL/L/LLｼﾘｰｽﾞ\nKQG2ｼﾘｰｽﾞ\nKFG2ｼﾘｰｽﾞ\nKPG/KPQｼﾘｰｽﾞ",null,"付属品","HF1B-Series カタログに準拠","同時梱包です。"]

{"sheet":"AF","index":2,"n_rows":52,"n_cols":17,"rows_kept":52,"cut":false,"hidden":false,"merged":[[10,9,10,14],[11,9,11,14],[0,0,0,6],[7,1,7,7],[10,1,13,5],[10,6,13,6],[10,7,13,7],[15,1,17,1],[15,2,17,5],[19,1,24,1],[19,2,24,5],[26,1,28,1],[26,2,28,2],[26,4,28,4],[26,5,28,5],[48,4,49,4],[48,5,49,5],[30,1,49,1],[30,2,49,2],[30,4,35,4],[30,5,35,5],[37,4,40,4],[37,5,40,5],[38,6,39,6],[42,4,43,4],[42,5,43,5],[45,4,46,4],[45,5,46,5]]}
["製品対象リストへ戻る"]
["エアフィルタ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)","50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]","[AC50]","[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","－","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","－","－","－"]
[null,null,null,null,null,null,"06","3／4",null,"－","－","－","●","●","－"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１/８",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１/４",null,"－","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","インジケータ","無記号","インジケータなし",null,"●","●","●","－","●","●"]
[null,null,null,null,null,null,"L","目詰まりチェッカ付",null,"●","●","●","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AFM","index":3,"n_rows":51,"n_cols":13,"rows_kept":51,"cut":false,"hidden":false,"merged":[[10,9,10,12],[11,9,11,12],[0,0,0,6],[7,1,7,7],[10,1,13,5],[10,6,13,6],[10,7,13,7],[15,1,17,1],[15,2,17,5],[19,1,23,1],[19,2,23,5],[25,1,27,1],[25,2,27,2],[25,4,27,4],[25,5,27,5],[47,4,48,4],[47,5,48,5],[29,1,48,1],[29,2,48,2],[29,4,34,4],[29,5,34,5],[36,4,39,4],[36,5,39,5],[37,6,38,6],[41,4,42,4],[41,5,42,5],[44,4,45,4],[44,5,45,5]]}
["製品対象リストへ戻る"]
["ミストセパレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１/８",null,"●","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１/４",null,"－","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","インジケータ","無記号","インジケータなし",null,"●","●","●","－"]
[null,null,null,null,null,null,"L","目詰まりチェッカ付",null,"●","●","●","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AFD","index":4,"n_rows":51,"n_cols":13,"rows_kept":51,"cut":false,"hidden":false,"merged":[[10,9,10,12],[11,9,11,12],[0,0,0,6],[7,1,7,7],[10,1,13,5],[10,6,13,6],[10,7,13,7],[15,1,17,1],[15,2,17,5],[19,1,23,1],[19,2,23,5],[25,1,27,1],[25,2,27,2],[25,4,27,4],[25,5,27,5],[47,4,48,4],[47,5,48,5],[29,1,48,1],[29,2,48,2],[29,4,34,4],[29,5,34,5],[36,4,39,4],[36,5,39,5],[37,6,38,6],[41,4,42,4],[41,5,42,5],[44,4,45,4],[44,5,45,5]]}
["製品対象リストへ戻る"]
["マイクロミストセパレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１/８",null,"●","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１/４",null,"－","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","インジケータ","無記号","インジケータなし",null,"●","●","●","－"]
[null,null,null,null,null,null,"L","目詰まりチェッカ付",null,"●","●","●","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AR","index":5,"n_rows":55,"n_cols":17,"rows_kept":55,"cut":false,"hidden":false,"merged":[[10,9,10,14],[11,9,11,14],[47,5,48,5],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[15,1,16,1],[15,2,16,5],[18,1,20,1],[18,2,20,5],[22,1,27,1],[22,2,27,5],[50,4,52,4],[50,5,52,5],[29,1,36,1],[29,2,36,2],[29,4,36,4],[29,5,32,5],[33,5,36,5],[38,1,52,1],[38,2,52,2],[38,4,39,4],[38,5,39,5],[41,4,42,4],[41,5,42,5],[44,4,45,4],[44,5,45,5],[47,4,48,4]]}
["製品対象リストへ戻る"]
["レギュレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。\n"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"➊"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)","50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]","[AC50]\n[AC60]","[AC50]\n[AC60]"]
[]
[null,"➋","逆流機能付",null,null,null,"無記号","逆流機能なし",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｋ","逆流機能付き",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➌","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➍","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","●","－"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➎","オプション",null,"a","圧力計","無記号","圧力計なし",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ","角形埋込式圧力計（リミットインジケータ付）",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｇ","丸形圧力計（リミットインジケータ付）",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｍ","丸形圧力計（カラーゾーン付）",null,"●","●","●","●","●","●"]
[null,null,null,null,null,"デジタル\n圧力スイッチ","Ｅ１","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線下取出し",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ２","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線上取出し",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ３","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線下取出し",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ４","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線上取出し",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➏","準標準",null,"b","設定圧力","無記号","０．０５～０．８５ＭＰａ設定",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"１","０．０２～０．２　ＭＰａ設定",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","排気機構","無記号","リリーフタイプ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ノンリリーフタイプ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","ハンドル向き","無記号","ハンドル下向き",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"Ｙ","ハンドル上向き",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と圧力計の単位表記：ＭＰａ",null,"●","●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板、注意銘板、圧力計の単位表記：ｐｓｉ／°Ｆ\nデジタル圧力スイッチ付：単位切換機能付／初期単位ｐｓｉ",null,"○","○","○","○","○","○"]
[null,null,null,null,null,null,"  ＺA 注2)","デジタル圧力スイッチ：単位切換機能付／初期単位ＭＰａ",null,"○","○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) 海外向けのみに適用",null,null,null,null,"○ 制約条件あり：注1）注2）参照\n"]

{"sheet":"AW","index":6,"n_rows":68,"n_cols":17,"rows_kept":68,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,13],[11,9,11,13],[15,1,16,1],[15,2,16,5],[18,1,20,1],[18,2,20,5],[22,1,27,1],[22,2,27,5],[29,1,40,1],[29,2,40,2],[29,4,31,4],[29,5,31,5],[33,4,40,4],[33,5,36,5],[37,5,40,5],[63,4,65,4],[63,5,65,5],[42,1,65,1],[42,2,65,2],[42,4,43,4],[42,5,43,5],[45,4,50,4],[45,5,50,5],[52,4,55,4],[52,5,55,5],[53,6,54,6],[57,4,58,4],[57,5,58,5],[60,4,61,4],[60,5,61,5]]}
["製品対象リストへ戻る"]
["フィルタレギュレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～h の各項目毎に１つずつ選択してください。\n"]
[null,"・オプション・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"➊"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]","[AC50]\n[AC60]"]
[]
[null,"➋","逆流機能付",null,null,null,"無記号","逆流機能なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｋ","逆流機能付き",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➌","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➍","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"➎","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","圧力計","無記号","圧力計なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ","角形埋込式圧力計（リミットインジケータ付）",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｇ","丸形圧力計（リミットインジケータ付）",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｍ","丸形圧力計（カラーゾーン付）",null,"●","●","●","●","●"]
[null,null,null,null,null,"デジタル\n圧力スイッチ","Ｅ１","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線下取出し",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ２","出力仕様：ＮＰＮ出力／リード線取出し仕様：配線上取出し",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ３","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線下取出し",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｅ４","出力仕様：ＰＮＰ出力／リード線取出し仕様：配線上取出し",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"➏","準標準",null,"c","設定圧力","無記号","０．０５～０．８５ＭＰａ設定",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"１","０．０２～０．２　ＭＰａ設定",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","ケース","無記号","ポリカーボネートケース",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１/８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１/４",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","排気機構","無記号","リリーフタイプ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ノンリリーフタイプ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"g","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"R","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"h","圧力単位","無記号","製品銘板、注意銘板、圧力計の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板、注意銘板、圧力計の単位表記：ｐｓｉ／°Ｆ\nデジタル圧力スイッチ付：単位切換機能付／初期単位ｐｓｉ",null,"○","○","○","○","○"]
[null,null,null,null,null,null,"  ＺA 注2)","デジタル圧力スイッチ：単位切換機能付／初期単位ＭＰａ",null,"○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) 海外向けのみに適用",null,null,null,null,"○ 制約条件あり：注1）注2）参照\n"]

{"sheet":"AFF","index":7,"n_rows":53,"n_cols":14,"rows_kept":53,"cut":false,"hidden":false,"merged":[[46,4,47,4],[46,5,47,5],[49,4,50,4],[49,5,50,5],[30,1,50,1],[30,2,50,2],[30,4,36,4],[30,5,36,5],[30,6,31,6],[38,4,41,4],[38,5,41,5],[39,6,40,6],[43,4,44,4],[43,5,44,5],[15,1,17,1],[15,2,17,5],[19,1,24,1],[19,2,24,5],[26,1,28,1],[26,2,28,2],[26,4,28,4],[26,5,28,5],[10,9,10,13],[11,9,11,13],[0,0,0,6],[7,1,7,7],[10,1,13,5],[10,6,13,6],[10,7,13,7]]}
["製品対象リストへ戻る"]
["ラインフィルタ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC50]","[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","－"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,null,"SUSケース",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１／４",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","インジケータ","無記号","インジケータなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","目詰まりチェッカ付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AM","index":8,"n_rows":53,"n_cols":14,"rows_kept":53,"cut":false,"hidden":false,"merged":[[46,4,47,4],[46,5,47,5],[49,4,50,4],[49,5,50,5],[30,1,50,1],[30,2,50,2],[30,4,36,4],[30,5,36,5],[30,6,31,6],[38,4,41,4],[38,5,41,5],[39,6,40,6],[43,4,44,4],[43,5,44,5],[15,1,17,1],[15,2,17,5],[19,1,24,1],[19,2,24,5],[26,1,28,1],[26,2,28,2],[26,4,28,4],[26,5,28,5],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,13],[11,9,11,13]]}
["製品対象リストへ戻る"]
["ミストセパレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC50]","[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","－"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,null,"SUSケース",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１／４",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","インジケータ","無記号","インジケータなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","目詰まりチェッカ付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AMD","index":9,"n_rows":53,"n_cols":14,"rows_kept":53,"cut":false,"hidden":false,"merged":[[46,4,47,4],[46,5,47,5],[49,4,50,4],[49,5,50,5],[30,1,50,1],[30,2,50,2],[30,4,36,4],[30,5,36,5],[30,6,31,6],[38,4,41,4],[38,5,41,5],[39,6,40,6],[43,4,44,4],[43,5,44,5],[15,1,17,1],[15,2,17,5],[19,1,24,1],[19,2,24,5],[26,1,28,1],[26,2,28,2],[26,4,28,4],[26,5,28,5],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,13],[11,9,11,13]]}
["製品対象リストへ戻る"]
["マイクロミストセパレータ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～fの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC50]","[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","－"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","オプション",null,"a","フロート式\nオートドレン","無記号","オートドレンなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｃ","N.C.(ノーマルクローズ）　無加圧時ドレン排出なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｄ","N.O.(ノーマルオープン）　無加圧時ドレン排出あり",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","準標準",null,"b","ケース","無記号","ポリカーボネートケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,null,"SUSケース",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"８","レベルゲージ付金属ケース",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ドレン排出口","無記号","ドレンコック付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｊ","ドレンガイド　１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,null,"ドレンガイド　１／４",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"Ｗ","ドレンコック、バーブ継手付",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","インジケータ","無記号","インジケータなし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","目詰まりチェッカ付",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"f","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"AMK","index":10,"n_rows":40,"n_cols":14,"rows_kept":40,"cut":false,"hidden":false,"merged":[[26,6,27,6],[33,4,34,4],[33,5,34,5],[36,4,37,4],[36,5,37,5],[15,1,17,1],[15,2,17,5],[19,1,24,1],[19,2,24,5],[26,1,37,1],[26,2,37,2],[26,4,31,4],[26,5,31,5],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,13],[11,9,11,13]]}
["製品対象リストへ戻る"]
["活性炭フィルタ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～cの各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC50]","[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"０１","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"０２","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"０３","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"０４","１／２",null,"－","－","●","－","－"]
[null,null,null,null,null,null,"０６","３／４",null,"－","－","－","●","－"]
[null,null,null,null,null,null,"１０","１",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"a","ケース","無記号","ポリカーボネートケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,null,"SUSケース",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"２","金属ケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"６","ナイロンケース",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"Ｃ","ケースガード付",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"６Ｃ","ケースガード付・ナイロンケース",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","圧力単位","無記号","製品銘板と注意銘板の単位表記：ＭＰａ／°Ｃ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板と注意銘板の単位表記：ｐｓｉ／°Ｆ",null,"○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"Y□(T)","index":11,"n_rows":28,"n_cols":16,"rows_kept":28,"cut":false,"hidden":false,"merged":[[17,1,18,1],[17,2,18,5],[20,1,21,1],[20,2,21,2],[20,4,21,5],[0,0,0,6],[12,1,15,5],[12,6,15,6],[12,7,15,7],[12,9,12,13],[13,9,13,13]]}
["製品対象リストへ戻る"]
["スペーサ・ブラケット付スペーサ"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,"200","300","400","500","600"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","スペーサ",null,null,null,"無記号","スペーサ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"T","ブラケット付スペーサ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","準標準",null,"ブラケットタイプ",null,"無記号","標準",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"1","ロングタイプ",null,"○","○","○","－","－"]
[null,null,null,null,"注1) ❷ブラケットでブラケット付スペーサを選択した場合のみ対象となります。",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]
[]
[]
[null,"組合せ注意事項"]
[null,"ブラケット付スペーサ・スペーサの配置について、以下の注意が必要です。"]

{"sheet":"VHS","index":12,"n_rows":45,"n_cols":16,"rows_kept":45,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,13],[11,9,11,13],[15,1,16,1],[15,2,16,5],[18,1,20,1],[18,2,20,5],[22,1,27,1],[22,2,27,5],[38,4,39,4],[38,5,39,5],[41,4,42,4],[41,5,42,5],[29,1,30,1],[29,2,30,2],[29,4,30,4],[29,5,30,5],[32,1,42,1],[32,2,42,2],[32,4,33,4],[32,5,33,5],[35,4,36,4],[35,5,36,5]]}
["製品対象リストへ戻る"]
["残圧抜き3ポート弁"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～e の各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、アルファベットの若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]",null,null,null,null,null,"\n"]
[null,null,null,null,null,null,null,null,null,20,30,40,"40(-06)","50"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ハンドル操作",null,null,null,"無記号","シングルアクション",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"W","ダブルアクション",null,"●","●","●","●","●"]
[]
[null,"❸","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","管接続口径",null,null,null,"01","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","－","－"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❺","オプション",null,"a","サイレンサ","無記号","なし",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"S","内蔵式サイレンサ付（EXHポート用）",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❻","準標準",null,"b","ハンドル色","無記号","赤",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｋ","黒",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","ハンドル材質","無記号","樹脂",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｍ","金属",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","流れ方向","無記号","流れ方向：左→右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","流れ方向：右→左",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"e","圧力単位","無記号","製品銘板の単位表記：ＭＰａ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"  Ｚ 注1)","製品銘板の単位表記：ｐｓｉ",null,"○","○","○","○","○"]
[null,null,null,null,"注1) ネジ種類NPT、海外向けのみに適用",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：注1）参照\n"]

{"sheet":"E□00","index":13,"n_rows":49,"n_cols":20,"rows_kept":49,"cut":false,"hidden":false,"merged":[[0,0,0,6],[9,9,9,13],[10,9,10,13],[14,1,16,1],[14,2,16,5],[18,1,25,1],[18,2,25,5],[9,1,12,5],[9,6,12,6],[9,7,12,7]]}
["製品対象リストへ戻る"]
["配管アダプタ"]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"200","300","400","500","600"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"12","１　１／４",null,"－","－","－","－","●"]
[null,null,null,null,null,null,"14","１　１／２",null,"－","－","－","－","●"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"営業企画室"]

{"sheet":"E□00L","index":14,"n_rows":25,"n_cols":14,"rows_kept":25,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,9,10,13],[11,9,11,13],[15,1,17,1],[15,2,17,5],[19,1,24,1],[19,2,24,5],[10,1,13,5],[10,6,13,6],[10,7,13,7]]}
["製品対象リストへ戻る"]
["L形配管アダプタ"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"200","300","400","500","600"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","－","●"]

{"sheet":"E□00T","index":15,"n_rows":25,"n_cols":14,"rows_kept":25,"cut":false,"hidden":false,"merged":[[19,1,24,1],[19,2,24,5],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,13],[11,9,11,13],[15,1,17,1],[15,2,17,5]]}
["製品対象リストへ戻る"]
["T形配管アダプタ"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"200","300","400","500","600"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","－","●"]

{"sheet":"Y□10","index":16,"n_rows":92,"n_cols":14,"rows_kept":92,"cut":false,"hidden":false,"merged":[[32,9,32,13],[20,1,22,1],[20,2,22,5],[24,1,28,1],[24,2,28,5],[30,1,31,1],[30,2,31,2],[30,4,31,5],[0,0,0,6],[15,1,18,5],[15,6,18,6],[15,7,18,7],[15,9,15,13],[16,9,16,13]]}
["製品対象リストへ戻る"]
["T形スペーサ"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"210","310","410","510","610"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","●","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","○","●","●","●"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","○","○","●"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","○","○"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"ボディタイプ",null,"無記号","標準",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"1","薄形",null,"●","●","●","●","●"]
[null,null,null,null,null,null,null,null,null,"● 制約条件なし"]
[null,null,null,null,null,null,null,null,null,"○ 制約条件あり：❹ボディタイプ「標準」のみ"]
[]
[]
[null,"組合せ注意事項"]
[null,"上記品番体系で、準標準仕様「1」を選択すると、従来品と面間寸法に互換性のある製品となります。"]
[null,"その場合、以下の組合せに注意が必要です。"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"又は"]

{"sheet":"Y□4","index":17,"n_rows":34,"n_cols":14,"rows_kept":34,"cut":false,"hidden":false,"merged":[[0,0,0,6],[17,1,20,5],[17,6,20,6],[17,7,20,7],[17,9,17,13],[18,9,18,13],[22,1,24,1],[22,2,24,5],[26,1,30,1],[26,2,30,5],[32,1,33,1],[32,2,33,2],[32,4,33,5]]}
["製品対象リストへ戻る"]
["クロススペーサ"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"24","34","44","54","64"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","○","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"ボディタイプ",null,"無記号","標準",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"1","前後ポート選択形",null,"●","●","●","●","－"]

{"sheet":"IS10M","index":18,"n_rows":98,"n_cols":14,"rows_kept":98,"cut":false,"hidden":false,"merged":[[15,1,26,1],[15,2,26,2],[15,4,16,4],[15,5,16,5],[18,4,20,4],[18,5,20,5],[22,4,23,4],[22,5,23,5],[25,4,26,4],[25,5,26,5],[0,0,0,6],[10,1,13,5],[10,6,13,6],[10,7,13,7],[10,9,10,13],[11,9,11,13]]}
["製品対象リストへ戻る"]
["圧力スイッチ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～d の各項目毎に１つずつ選択してください。\n"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"20","30","40","50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","準標準",null,"a","設定圧力範囲","無記号","0.1~0.4MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"6 注1)","0.1~0.6MPa",null,"○","○","○","○","○"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","リード線長さ","無記号","0.5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","3m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Z","5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","目盛板圧力単位","無記号","MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｐ 注2)","MPa・psi併記",null,"○","○","○","○","○"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","ボディタイプ","無記号","標準",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"1","薄形",null,"●","●","●","●","●"]
[null,null,null,null,"注1) ❷準標準で\"6P\"を選択した場合、設定圧力範囲は0.2～0.6MPa(30～90psi)になります。",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) 海外向けのみに適用。",null,null,null,null,"○ 制約条件あり：注1）注2）参照\n"]
[]
[]
[null,"組合せ注意事項"]
[null,"上記品番体系で、準標準仕様「1」を選択すると、従来品と面間寸法に互換性のある製品となります。"]
[null,"その場合、以下の組合せに注意が必要です。"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"又は"]

{"sheet":"IS10T","index":19,"n_rows":36,"n_cols":14,"rows_kept":36,"cut":false,"hidden":false,"merged":[[10,9,10,13],[11,9,11,13],[19,1,23,1],[19,2,23,5],[15,1,17,1],[15,2,17,5],[10,7,13,7],[0,0,0,6],[25,1,33,1],[25,2,33,2],[25,4,26,4],[25,5,26,5],[28,4,30,4],[28,5,30,5],[32,4,33,4],[32,5,33,5],[10,1,13,5],[10,6,13,6]]}
["製品対象リストへ戻る"]
["Ｔ形スペーサ付圧力スイッチ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～c の各項目毎に１つずつ選択してください。\n"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"20","30","40","50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]","[AC40-06]","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","●","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","●","●"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"a","設定圧力範囲","無記号","0.1~0.4MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"6 注1)","0.1~0.6MPa",null,"○","○","○","○","○"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","リード線長さ","無記号","0.5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","3m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Z","5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","目盛板圧力単位","無記号","MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｐ 注2)","MPa・psi併記",null,"○","○","○","○","○"]
[null,null,null,null,"注1) ❹準標準で\"6P\"を選択した場合、設定圧力範囲は0.2～0.6MPa(30～90psi)になります。",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) 海外向けのみに適用。",null,null,null,null,"○ 制約条件あり：注1）注2）参照\n"]

{"sheet":"IS10L","index":20,"n_rows":40,"n_cols":14,"rows_kept":40,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,9,10,13],[11,9,11,13],[10,1,13,5],[10,6,13,6],[10,7,13,7],[15,1,17,1],[15,2,17,5],[36,4,37,4],[36,5,37,5],[19,1,24,1],[19,2,24,5],[26,1,37,1],[26,2,37,2],[26,4,27,4],[26,5,27,5],[29,4,31,4],[29,5,31,5],[33,4,34,4],[33,5,34,5]]}
["製品対象リストへ戻る"]
["Ｌ形配管アダプタ付圧力スイッチ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～d の各項目毎に１つずつ選択してください。"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,20,30,40,"50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]\n","[AC30]\n","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","●","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"a","設定圧力範囲","無記号","0.1~0.4MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"6 注1)","0.1~0.6MPa",null,"○","○","○","○","○"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","リード線長さ","無記号","0.5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","3m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Z","5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","目盛板圧力単位","無記号","MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｐ 注2)","MPa・psi併記",null,"○","○","○","○","○"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","取付位置","無記号","右",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","左",null,"●","●","●","●","●"]
[null,null,null,null,"注1) ❹準標準で\"6P\"を選択した場合、設定圧力範囲は0.2～0.6MPa(30～90psi)になります。",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) 海外向けのみに適用。",null,null,null,null,"○ 制約条件あり：注1）注2）参照\n"]

{"sheet":"IS10E","index":21,"n_rows":42,"n_cols":14,"rows_kept":42,"cut":false,"hidden":false,"merged":[[0,0,0,6],[10,9,10,13],[11,9,11,13],[10,1,13,5],[10,6,13,6],[10,7,13,7],[15,1,17,1],[15,2,17,5],[38,4,39,4],[38,5,39,5],[19,1,26,1],[19,2,26,5],[28,1,39,1],[28,2,39,2],[28,4,29,4],[28,5,29,5],[31,4,33,4],[31,5,33,5],[35,4,36,4],[35,5,36,5]]}
["製品対象リストへ戻る"]
["配管アダプタ付圧力スイッチ"]
[]
[]
[]
[]
[]
[null,"・オプション・準標準は、a～d の各項目毎に１つずつ選択してください。\n"]
[null,"・準標準記号は、数字、アルファベットの順で、若い順に並べて表示します。"]
[]
[null,null,null,null,null,null,"記号","内容",null,"❶"]
[null,null,null,null,null,null,null,null,null,"ボディサイズ\n[適用ACサイズ]"]
[null,null,null,null,null,null,null,null,null,"20","30",40,"50","60"]
[null,null,null,null,null,null,null,null,null,"[AC20]","[AC30]","[AC40]\n","[AC40-06]\n","[AC50]\n[AC60]"]
[]
[null,"❷","ねじ種類",null,null,null,"無記号","Ｒc",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｎ","ＮＰＴ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｆ","Ｇ",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,"❸","管接続口径",null,null,null,"01","１／８",null,"●","－","－","－","－"]
[null,null,null,null,null,null,"02","１／４",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"03","３／８",null,"●","●","●","－","－"]
[null,null,null,null,null,null,"04","１／２",null,"－","●","●","－","－"]
[null,null,null,null,null,null,"06","３／４",null,"－","－","●","●","●"]
[null,null,null,null,null,null,"10","１",null,"－","－","－","●","●"]
[null,null,null,null,null,null,"12","１　１／４",null,"－","－","－","－","●"]
[null,null,null,null,null,null,"14","１　１／２",null,"－","－","－","－","●"]
[null,null,null,null,null,null,"＋"]
[null,"❹","準標準",null,"a","設定圧力範囲","無記号","0.1~0.4MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"6 注1)","0.1~0.6MPa",null,"○","○","○","○","○"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"b","リード線長さ","無記号","0.5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"L","3m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Z","5m",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"c","目盛板圧力単位","無記号","MPa",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｐ 注2)","MPa・psi併記",null,"○","○","○","○","○"]
[null,null,null,null,null,null,"＋"]
[null,null,null,null,"d","取付位置","無記号","右端用",null,"●","●","●","●","●"]
[null,null,null,null,null,null,"Ｒ","左端用",null,"●","●","●","●","●"]
[null,null,null,null,"注1) ❹準標準で\"6P\"を選択した場合、設定圧力範囲は0.2～0.6MPa(30～90psi)になります。",null,null,null,null,"● 制約条件なし\n"]
[null,null,null,null,"注2) 海外向けのみに適用。",null,null,null,null,"○ 制約条件あり：注1）注2）参照\n"]

{"sheet":"E□00E","index":22,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,6],[9,1,10,5],[9,6,10,6],[9,7,10,7],[12,1,14,1],[12,2,14,5]]}
["製品対象リストへ戻る"]
["エンドプレート"]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"記号","内容"]
[]
[]
[null,"❶","ボディサイズ",null,null,null,200,"AC20-D用"]
[null,null,null,null,null,null,"300","AC30-D用"]
[null,null,null,null,null,null,"400","AC40-D用"]